This document will be updated as customer ask questions about building and using the kit.

Please refer to the IBM Technical Reference Manual before sending questions by email.

-----------

Question: Regards the small 47nF and 47pF capacitors... Should they both be mounted with
one lead in a central hole, and the other lead in either of the side holes?

Answer: Yes.  These capacitors are non-polarized, which means there are no "+"
or "-" leads: They can be mounted either way.

-----------

Question: Is the U100 socket supposed to be empty?

Answer: Yes. This socket location is a spare location that was included by the IBM
designers 'just in case' they needed to add another IC at the last minute.

-----------


MTM
March, 2017