Ad Lib Multimedia inc.
580, Grande-Allee Est, suite 40
Quebec, QC. Zip Code : G1R 2K2
Telephone : (418) 522-6100

                    Ad Lib Multimedia, Quebec

Device Driver installation for OS2 V3.00 (or later).

Make sure that OS/2 is fully installed and functional BEFORE installing
an AdLib Sound Driver!

STEP 1 : Go to the diskette and execute de CLOCKFIX.BAT bath file.

STEP 2 : Open the "MULTIMEDIA - ICON VIEW" and
         start the "multimedia application install".

STEP 3 : Select Source "A:" or anywhere is your installation disk.

STEP 4 : Select which driver you want. Accept all defaults values.

NOTE : Because the ADLIB sound card is plug and play, the OS2 drivers
       will read the PnP BIOS inside the card in order to obtain
       the corrects values for IRQ, DMA et I/O ports.

       You can, at any time, start again the installation programs.
       If you forget to start the CLOCKFIX batch file, you can do it
       any time later.

The installation program will make 3 new icons inside the multimedia
group :
        1 - "MIDI" for playing MIDI files with the OPL3 chips.
        2 - "MIDI 2" for playing MIDI files with the WAVE TABLE.
        3 - "Digital Audio" for creating and modifying your own sounds.

NOTE : The volume control dont work with the "MIDI 2" icon. It's because
       the volume should be ajusted by standard midi message instead of
       direct register manipulation of some I/O ports. Sorry, it's better
       to have volume adjustment button directly on your speaker! May be
       you could find a console program that use standard MIDI commands.

ADLIB device driver Version 1.5
technical OS2 support : Christian Gingras

Release of MAY 1996.

