


Install this driver on Windows NT 3.5 or greater.  Use the Windows NT 
Control Panel, Drivers option to automatically install this driver and 
audio control apps.  This driver does not read Plug and Play system 
BIOS.  So the user  must place the I/O address, Interrupt and DMA 
channels into unused system resources.  


      - CS32BA11 Version 1.0 driver is not compatible with Win NT 3.1.
        Must be Win NT 3.5 or later.

      - ASB Special Edition DOES NOT SUPPORT IRQ 10 or DMA 0,
	The Install program will force you to make another choice.

