
=== ES1869 SOFTWARE WAVETABLE DRIVER ===

 This driver is only for windows 95 OSR2 version or above.
 You have better use Pentium or above system.

 --Installation--
1. Please the follow the steps for remove old ES1869 driver first 
   a. Remove all the ESS items in "Sound, Video and game controllers"
      under My Computer -> Control Panel -> System -> Device Manager.
   b. Deletee the "essoemsetup.inf" under <Windows95 root>\system\inf\other. 
     (Note: inf is hidden sub-directory, please display it first.(see your
            Windows 95 User Guide))
   c. Deletee all the "ES*.*" files under <Windows95 root>\system.

2. Restart Windows 95 OSR2.

3. When Update Device Wizard pops up and announces 
   "This Wizard will complete the installation of ESS ES1869 Plug and Play 
    AudioDrive."  Please follow the process of "Installing the Sound Card 
   Software with Windows 95 OSR2" on manaul to install. 
   But locate driver to d:\driver\ess\1869\swtable

4. After successful installation, you can see new adding 
   "Internal ESS software wavetable" item under 
   My Computer -> Control Panel -> Multimedia -> MIDI.
   Choose it!  You can play midi by wavetable effect!
 