Installation Instructions For audioblitz stereo 16+
Model A3300/A3400
Drivers and utilities for DOS and Windows 3.1x only
Drivers for Win95 and NT are not available for this 
product.

There are 2 files in this archive;
ab16_d1.zip
ab16_d2.zip

These archives contain subdirectories with files.
In order to extract these files properly they must
be extracted to 2 separate floppy disks. 
USE THE PKUNZIP.EXE "-D" extraction switch when 
extracting to floppy. The syntax is as follows;

From a DOS prompt enter PKUNZIP -D (file name) (destination)
example;
PKUNZIP -D ab16_d1.zip a:

This will extract all the files in that archive to 
a floppy disk in drive A. 

INSTALLING THE SOFTWARE

1) Insert disk 1 into drive a: (or b: if applicable)
2) From the DOS prompt type setup and press enter.
3) You will see a setup screen
the screen allows you to choose your options.
