             GraphicsENGINE Autodesk ADI4.2 (Protected-mode)
                          display list driver.

Features:
 The ADI 4.2 driver is used for AutoCAD Release 10/11/12, AutoShade.
 2.0/2.1 and 3D Studio 1.0/2.0.
 32 BITS DISPLAY FOR  NO REGEN\OPERTION.
 Bird_Eye and Edge-Pan features for convenient zooms and pans.

Hardware Requirements:
 * 286 or better CPU.
 * GraphicsENGINE  board.
 * 80X87.

Restriction:
 * The ADI4.2 driver is protected mode only.
 * Resolutions which require 2MB are not supported at this time.
 * Rendering problems occure in 15,16 and 24 bit resolutions.
 * In 800x600 and 1024x768 resolutions,text does not display
   in the bottom of the window after doing a DIR from a flipscreen.
 * With the side menu disabled, the S3 logo may appear in unexpected
   places.

Resolution:
  640 X  480    256 COLORS 
  640 X  480  32768 COLORS (Rendering Mode)
  640 X  480  65535 COLORS (Rendering Mode)
  640 X  480  16.7M COLORS (Rendering Mode)
  800 X  600     16 COLORS 
  800 X  600    256 COLORS 
 1024 X  768     16 COLORS 
 1024 X  768    256 COLORS 
 1280 X  960     16 COLORS 
 1280 X 1024     16 COLORS 

DRIVER INSTALLATION FOR USE WITH AUTOCAD RELEASE 11, 12:

 1. Copy driver (RCP_S3.EXP) to a convenient location.
    The file INSTALL.EXE can be used to copy the
    driver by first logging onto the desired drive and
    directory  then typing
               A:\> install

    Then select INSTALL's \Autodesk ADI4.2 (Protected Mode) \ menu,
    press ENTER key and complete the installation.
    INSTALL will copy the appropriate files to your default directory.

 2. Set the environment variable  ACADDRV=\to point to the
    Aquila sub-directoryand load files into Aquila sub-directory as well.
     Example:
     ACAD 12     SET ACADDRV= C:\ACAD\Aquila\;C:\ACAD\DRV\
     ACAD 11  SET DSPADI = C:\ACAD\Aquila\RCP_S3\
                 SET RCPADI = %DSPADI%
                 SET RDPADI = %DSPADI%

    If desired, this command can be placed in the AUTOEXEC.BAT file.

 3a. Set Acad device to  Aquila 4.2\in the AutoCAD display device
     configuration menu for AutoCAD 12.
  b. Set Acad device to  ADIP386 V4.0/4.1 Display\in the AutoCAD
     display configuration menu for AutoCAD 10 and 11.

 4. Select the desired mode from the list of available modes in
    the ACAD configuration menu.

 5. Configure options such as dual screen operation (if your system has 
    the capability), menu colors, Graphics Flip Screen feature, mouse,
    printer and plotter as needed. The GFS option enables the AutoCAD 
    text screen to be displayed in the center of the graphics screen.
    This will eliminate the mode switching delay which are found in most
    multi frequency monitors. Do not use this option if a TSR program is 
    being used.

DRIVER INSTALLATION FOR USE WITH AUTOSHADE 2.X:

 1. Delete  \shade2\shade.cfg\

 2. Set environment variables in  \autoexec.bat : as we did in ADI4.1

 3. Reboot machine.

 4. Run  shade /R\from  \shade2\directory.

 5. Select pointing device.

 6. Select  P386 Autodesk Device Interface display driver .

 7. Choose a mode NOT marked as  Disabled .


 8. Answer  YES\3 (three) times-
    a. YES, display and AutoShade rendering devices share a single screen.
    b. YES, display and RenderMan rendering devices share a single screen.
    c. YES, FLIP SCREEN does require a redraw.

 9. Select a rendering hardcopy device.

10. Quit, and the configuration will be saved.

DRIVER FOR 3D STUDIO 2.0 CONFIGURATION,
 1. Go to  \3ds \sub-directory, and edit the file  3DS.SET .

 2. Change the line which started with \DEFAULT-DISPLAY = VGA320X200\
    to  DEFAULT-DISPLAY = RCP_S3\and  MATERIAL-DISPLAY = VGA320X200\.
    to  MATERIAL-DISPLAY = RCP_S3 .

 3. Change  MAIN-DISPLAY = \to  MAIN-DISPLAY = RCP_S3 . Delete any 
    leading semicolon (;) that may be present. 

 4. Delete the file  3DADI.CFG\if present. 

 5. Run  3DS\and select  ADI main Display .

 6. At  ADI MEDIT\select a 256 colors resolution.

 7. Answer rest question of the screen.
    (Detail in the readme.txt)
