AVANCE LOGIC, ALG2032/2064 WINDOWS 3.1/AutoCAD DRIVER VERSION ALG32.A1.30

Subject:

MS Windows/3.1 and DCI display drivers.
AutoCAD R12/R13/3Dstudio driver.

Date:

Aug 2, 1996.

Supporting modes:

1.  640X480 16 color
2.  640X480 256 color
3.  640X480 64K color
4.  640X480 16M color
5.  800X600 16 color
6.  800X600 256 color
7.  800X600 64K color
8.  1024X768 16 color
9.  1024X768 256 color
10.  1024X768 64K color (2MB memory required)
11.  1280X1024 16 color
12.  1280x1024 256 color (2MB memory required)

Refresh rate and mode change can be made by running VMASTER.EXE under ALG2032/64
directory.

Procedure:

AVANCE LOGIC WINDOWS 3.1 HIGH RESOLUTION DRIVERS INSTALLATION PROCEDURE:

   * IF YOU HAVE PREVIOUS DRIVER DISKETTE, PLEASE SETUP VGA MODE, THEN
     START THE WINDOWS AND DELETE AVANCE LOGIC ICON GROUP. RESTART
     INSTALLATION FROM STEP 7.

   * FOR FIRST TIME USER PLEASE START FROM STEP 1.6

   INSTALLATION PROCEDURE:

    1. CHANGE DIRECTORY TO WINDOWS 3.1 AND TYPE "SETUP".

    2. SELECT "DISPLAY" AND "ENTER".

    3. CHANGE TO "VGA" AND "ENTER".

    4. FOLLOW THE INSTRUCTIONS ON THE SCREEN TO FINISH THE WINDOWS
       SETUP PROGRAM.

    5. RESTART YOUR WINDOWS 3.1 PROGRAM BY TYPING "WIN" AT DOS PROMPT.

    6. PUT THE DISTRIBUTION DISKETTE INTO DRIVE A: (OR B:)

    7. SELECT "RUN" AT PULL DOWN MENU OF PROGRAM MANAGER AND MOVE
       THE CURSOR TO "RUN".

    8. ENTER THE FILE NAME FOR AVANCE LOGIC WINDOWS DRIVER INSTALLATION
       PROGRAM A:\SETUP.EXE (OR B:\SETUP.EXE IF THE INSTALLATION DISK IS
       IN DRIVE B:).

    9. RUN VMASTER TO SELECT RESOLUTION, COLOR DEPTH, AND REFRESH RATE WITHOUT
       QUITTING WINDOWS.


(1) ACAD R12 (2) ACAD R13 (3) 3D STUDIO
ßßßßßßßßßßßßßßßßßßßßßßßßßßßßßßßßßßßßßßß

 First, copy DSPALI42.EXP to DRV Subdirectory under your AutoCAD directory.

 1. Make sure the AutoCAD works fine with VGA.
 2. Begin AutoCAD with the reconfigure switch by typing
               ACAD -R
 3. Select option 3 ("Configured Video Display").
 4. Type Y at the "Do you want to select ..." message to
    display the available video options for AutoCAD.
 5. Select "ALI VGA ADI v4.2, by Avance Logic, Inc".
 6. Select display resolution you want.
 7. Follow the directions provided by the AutoCAD program to complete
    your AutoCAD configuration.
 8. Save your new changes.
    (Now, you complete re-configuration )
 9. The AutoCAD will start.

NOTE
ßßßß
 *. Every time you reboot your system,
    If need to change the resolution just type ACAD -R, otherwise start
    the AutoCAD as usual.

 *. The available drivers show on your ALG2032/2064 utility disk as following:
    ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
     ADI Ver.    Resolution
    ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
     ADI v4.2     640x480/256colors
     ADI v4.2     800x600/256colors
     ADI v4.2    1024x768/256colors
     ADI v4.2   1280x1024/256colors              (required 2MB)
    ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ


3D Studio
ßßßßßßßßß
 1. Use SET command at the DOS prompt, or your AUTOEXEC.BAT file:
        SET RCPADI = (3D-Studio drive)\DSPALI42.EXP)
 2. Copy DSP25128.EXP to your 3D Studio DRIVERS directory, and reconfig
    your 3DS, select the mode you want to run at your system.

  The 2032/2064 new display modes:
              --   640x480  256-color
              --   800x600  256-color
              --  1024x768  256-color
              -- 1280x1024  256-color   (required 2MB)

NOTE
ßßßß
  Check 3D Studio manuals for additional information
  to configure program for ALG2032/2064 new drivers.
