
This READ.ME contains important supplements to your "WaveRunner Digital
Modem Installation and Testing Instructions."  Additional information
and software updates may be obtained from the IBM Personal Computer
Company Bulletin Board System via a modem by calling 1-919-517-0001.
Information may also be obtained over the INTERNET by anonymous FTP to
www.raleigh.ibm.com and accessing subdirectory pub/standards/waverun.


INSTALLATION and TESTING:
=========================


Installation Prerequisites:
----------------------------------

WaveRunner is designed to run in a Windows 3.1 environment with at
least 4 MB of RAM and in a Windows for Work Groups 3.11 environment
with at least 6 MB of RAM.  5 MB of available hard disk space is
required.

This release of the Windows version of WaveRunner Digital Modem will not
operate in a Win-OS2 session.


Updating the Reference Diskette:
--------------------------------------------


If you are installing WaveRunner in a PS/2 Model P70, the Reference
Diskette must be Version 1.04 or higher to successfully update from the
Startup Option Diskette.


Testing the WaveRunner Adapter for ISA:
---------------------------------------------------------


If the NT1 Loopback Test Fails:
-------------------------------------------

The following conditions may result in a failure of the NT1 Loopback
Test:

1)  The NT1 does not support the S&Q maintenance channel.
    Check the NT1 user manual.  If the S&Q channel is not supported,
    this test cannot be run.

2)  The ISDN cable is defective.  Replace the cable and rerun the test.

3)  The adapter is not correctly connected to the NT1.  Check all the
     cable connections from the adapter to the NT1 and from the NT1 to
     the ISDN line.

4)  The NT1 is not powered on.

5)  The NT1 is not connected to an active ISDN line.  Some NT1 models
    cannot perform S&Q loopbacks unless connected to an active line.

6)  The NT1 is defective.  NT1 error lights may indicate a problem.
    Check the NT1 user manual for troubleshooting information.

7)  The ISDN line is not active.

If all the above conditions have been eliminated, your adapter may
need to be replaced.


Test does not advance past "Performing Test 26":
------------------------------------------------------------------

When running diagnostics, if your computer screen does not advance past
"Performing Test 26," the DMA switch setting (Switch Block S2)
may not match the setting specified in the diagnostics setup.  Make sure
that the DMA channel specified in the diagnostics setup matches the
DMA channel selected on the adapter.


HELPFUL HINTS FOR SELECTED COMMUNICATIONS APPLICATIONS:
============================================================


Configuring your Communications Application
-----------------------------------------------------------------

Configure your communications application for a Hayes compatible modem
or Mwave compatible modem.  Also, configure the application to use the
same COM Port for which WaveRunner is configured.


PROCOMM PLUS For Windows
----------------------------------------------

To ensure proper application-to-application connections using ProComm,
configure ProComm as follows:

       Default Baud Rate:  115200 bps
       Auto Baud Select :  Off (NOT selected)

Problems avoided with this setup:

1) Asynchronous communication devices cannot connect at speed greater
   than the UART (baud) speed.  To connect at 64000, the UART must be
   configured for 64000 or greater.  115200 bps is the only choice in
   ProComm that allows V.120 to connect.

2) With ProComm Auto Baud Detect on, ProComm will only make
   connections at its pre-anticipated (exact) speeds of 300, 1200,
   2400, 9600, 14400, 19200, 38400, or 57600 bps.

   If the line connects at 56000 or 64000, ProComm will not recognize
   the connect speed and disconnect the call.  This problem can be
   avoided by turning Auto Baud Detect OFF in the Modem setup section
   of the advanced connection setup as described above.


HyperACCESS For Windows
-----------------------------------------

Answer Text:

HyperACCESS 3.0 and HyperACCESS 3.1 are unable to detect 56000 & 64000
bps line speeds.  You may get the first CONNECT message, then an
"unable to determine baud rate" message or a DISCONNECT.  Add the
following lines to the section labeled "AdjustBaudRate3" in the script
file ANSWER.HP:

      if equal(MiscInt2,56000) goto SetBaudAndSynch
      if equal(MiscInt2,64000) goto SetBaudAndSynch

Updated answer text files are available on the PC Company Bulletin
Board in the files "ANSWER30.HP and "ANSWER31.HP". Perform a search on
"waverunner" to locate the files.

User Defined Modem:

Under the Hardware option, select the user-defined modem.  Run modemdef
from the ALT+R prompt to define the modem.  The settings should be
defined as follows:

      Call setup commands   = ATE1V1Q0X3&C1&D2
      Answer setup commands = ATE1V1Q0X3S0=1
      Dial command          = ATDT
      Hangup command        = ATH0
      Send answer setup commands even if CD high = NO
      Toggle DTR to hangup  = Yes
      Use hdw handshaking <rts/cts> flow control = YES

The last setting is a must for error correction.  See Appendix A User
Defined Modem (page 277) of the HyperAcess 5 manual for more details.


Trio DataFaxProgram for Windows:
-------------------------------------------------

By default Trio will add the DataFax Server, DataFax Captive, and
DataFax Faxoffice program icons to the startup group.  This can become
a nuisance if you do more modem functions than Fax.  The user can elect
not to place these icons in startup by unchecking the button "Modify
WIN.INI".

Class 2 Fax uses the COM port for transmissions.  If the Fax server is
in the STARTUP program group, it will configure the modem for fax.
Other COM port applications will not have access to the modem until the
FAX server is unloaded.  The modem application must be running before
using Class II FAX.

To use COM port applications the FAX server must be unloaded and the
Modem application reloaded.

In the case of MCI FAX, most WaveRunner DSP resources are used by the
FAX tasks and there will be no room for modem DSP tasks on the adapter
until fax is unloaded.


CrisNet
-----------

CrisNet is a Real Estate application

The ISDN.INI file is used by ISDN.EXE to run Comm Programs using
WaveRunner.  ISDN.EXE ensures that the correct drivers are loaded prior
to execution. The following parameters must be specified.

     PORT=Program & Path of ISDN Port Manager
     MODEM=Program & Path of ISDN Modem application
     ISDN=Program & Path of TCP/IP ISDN Driver
     FAX=Program & Path of Data Fax Server (TRIO)

Some of the names of the WaveRunner executable programs have been
altered and appropriate changes must be made in the
CrisNet control files.

To use ISDN.EXE, add the desired ProgramName(ID) to ISDN.INI followed
by "=", the type of WaveRunner application (MODEM, ISDN, or FAX), a
comma, and then the Path and Program of the subject communication
program.  ISDN stands for TCP/IP.

     [WAVERUNNER]
     LOADER=C:\WAVERUN\wrportmw.EXE
     PORT=C:\WAVERUN\wrportmw.EXE
     MODEM=C:\WAVERUN\MODEM\wrmodemw.EXE
     ISDN=C:\WAVERUN\ADLC\wradlcw.EXE
     FAX=C:\DATAFAX\WINSERVE.EXE

     SFVAR Comm Programs

     CRISNET=ISDN,C:\CRISNET\CRISNET.EXE
     SFVBL=MODEM,C:\SFVBL\SFVBL.PIF
     RMAP=MODEM,C:\RMAP2\RMAP.PIF
     WW=FAX,C:\WINWORD\WINWORD.EXE
     PCPLUS=MODEM,C:\PCPLUS\PCPLUS.PIF
     OLDCRIS=MODEM,C:\WINDOWS\TERMINAL.EXE C:\WINDOWS\SFVAR.TRM


LAN Distance Remote for Windows
-------------------------------------------------

If the WaveRunner PCMCIA COM Port is not listed while installing LAN
Distance, continue installing LAN Distance with the incorrect COM Port
selected.  Restart the workstation and Windows and perform the
following steps to add the correct COM Port:

   Start LAN Distance
   Select Settings
   Select Ports
   Delete the incorrect COM Port
   Restart the workstation and Windows
   Start the WaveRunner Async-to-Sync Modem and the ISDN Port Monitor
   Start LAN Distance
   Select Settings
   Select Ports
   Add the correct COM Port
   Select Modem
   Assign the IBM Mwave WaveRunner Digital Modem
   Save the information
   Restart the workstation

A message may be received indicating that not enough memory is
available to load the applications.  This can be caused by DOS
device drivers and Windows device drivers being loaded into system
memory.  Review your DOS "config.sys" file and Windows Control Panel
Drivers configuration to eliminate unnecessary drivers.


