2007/08/08 Wrote by Kidd Wang.
T60H976.00 XB63 Released for xp-32/64bits: 
1.WHQL driver v5.3.0.67.(Negative-Pole LED)
  Silent insatllation: c:\Atheros-driver\setup /s or double click this file(SilentInstall.bat).
2.Update to IS12 to fix unclean remove oem*.inf issue.
3.NDIS: Increase WOW keep alive threshold from 16 to 255.
4.NDIS: Fixed BSOD when switching HW radio on\off.
