
To install your Windows(r) Vista(tm) printer & TWAIN scanner Drivers for the AL-2040CS:
 
1.       Make sure your AL-2040CS- IS NOT - connected to the PC.
2.       Double click the setup.exe file to start the installation process. 
3.       The setup.exe file will install all the necessary driver files into the appropriate folders. 
4.       After the installation is completed, turn on the AL2040CS and connect it to the PC.  
5.       Windows(r) Vista(tm), seeing a USB printer attached to it, will prompt you to continue to install the necessary drivers.  
6.       Choose the default settings of searching for the best driver 
7.       Windows(r) Vista(tm) will find the correct files, and finish installing the AL2030CS.   
 
If you have installation questions please contact 800-BE-SHARP

