



  			  A g e n t   O r a n g e

		   entry to assembly97 - demo competition



     	Requires a Pentium with 12Mb of physical available memory,
	preferrably 10ns SDRAMS. 320x240x16bpp is nice mode to have in
	your videocard but 640x480x16bpp also works, provided the chipset
	is VGA register level compatible (hardware stretching).


	Special thanks to Juha Koiste for 3D modelling <g>











		(c) Zog, H„mymies & Ovela-Jussi 1996-1997.
