miniport_471.txt file for AMD AGP Miniport Driver Version 4.71 for Windows 98/98SE/
  Millennium Edition(ME)

(c) Copyright 2000 Advanced Micro Devices, Inc.  All rights reserved.  

LIMITATION OF LIABILITY: THE MATERIALS ARE PROVIDED AS IS WITHOUT ANY EXPRESS OR
IMPLIED WARRANTY OF ANY KIND INCLUDING WARRANTIES OF MERCHANTABILITY, 
NONINFRINGEMENT OF THIRD-PARTY INTELLECTUAL PROPERTY, OR FITNESS FOR ANY PARTICULAR
PURPOSE. IN NO EVENT SHALL AMD OR ITS SUPPLIERS BE LIABLE FOR ANY DAMAGES 
WHATSOEVER (INCLUDING, WITHOUT LIMITATION, DAMAGES FOR LOSS OF PROFITS, BUSINESS
INTERRUPTION, LOSS OF INFORMATION) ARISING OUT OF THE USE OF OR INABILITY TO USE
THE MATERIALS, EVEN IF AMD HAS BEEN ADVISED OF THE POSSIBILITY OF SUCH DAMAGES.
BECAUSE SOME JURISDICTIONS PROHIBIT THE EXCLUSION OR LIMITATION OF LIABILITY FOR
CONSEQUENTIAL OR INCIDENTAL DAMAGES, THE ABOVE LIMITATION MAY NOT APPLY TO YOU.
AMD does not assume any responsibility for any errors which may appear in the 
Materials nor any responsibility to support or update the Materials. AMD
retains the right to make changes to its test specifications at any time, 
without notice. NO SUPPORT OBLIGATION: AMD is not obligated to furnish, support, 
or make any further information, software, technical information, know-how, or 
show-how available to you.
U.S. GOVERNMENT RESTRICTED RIGHTS: The Materials and documentation are provided 
with RESTRICTED RIGHTS. Use, duplication or disclosure by the Government is 
subject to restrictions as set forth in FAR52.227014 and DFAR252.227-7013, et
seq., or its successor. Use of the Materials by the Government constitutes
acknowledgment of AMD’s proprietary rights in them.


REQUIREMENTS:
Motherboard with AMD-751 System Controller (Northbridge)
Windows 98/98SE/ME (not for use on NT 4.0 or Windows 2000)
AGP video card


INSTALLATION INSTRUCTIONS:
To run the standard installation program, double-click on miniport_471.exe
1. A Welcome installation window is displayed, press Next to install, Cancel to 
quit.
2. After installation a Finish installation window is displayed, press Finish. 
3. The setup program installs the driver and .inf file and updates the system 
registry.
4. REBOOT the system to load the driver. 

To install the driver in silent mode without prompts:
1. At the command line in a DOS box, for example type:   miniport_471 /s
2. The installation of the driver runs silently. The setup program installs the 
driver and .inf file and updates the system registry.
3. REBOOT the system to load the driver.  

To check the version of the driver:
1) Using explorer, right click on the setup or driver file, select "Properties".
2) Select the "Version" tab.  The "File Version" field will be displayed.


REVISION HISTORY:
***** Version 4.71 *****
- Fixed an issue with Hibernation support

***** Version 4.61 *****
- Added AGP bridge driver to address PCI Cardbus controller issue
- Added ACPI/APM support for AGP bridge driver

***** Version 4.45 *****
- Changed behavior when errant video driver writes to an invalid GART table entry

***** Version 4.44 *****
- Initial release