





     JRTELE is a telecommunications program written specifically for the
 PCjr.  It requires 128K of memory, a disk drive, and either an IBM internal
 modem for the PCjr or a Hayes-compatible modem (external or internal).

     New features of JRTELE.COM Version 2.1 are:
          . Use of transparency or double control-N uploading with the IBM
            internal modem.
          . Ability to save the screen to the log file.

     JRTELE documentation is in the file JRTELE.DOC.  It may be printed using
 the DOS command:  copy jrtele.doc prn.
