; --------------------------------------------------------------
; Registry setting note
; --------------------------------------------------------------

Note:The following registry keys can be set by ThBDAConsole.exe as well.


1. For previous MCE2005 setting (DVB-T only),
   If MCE2005 Emerald Rollup-2 is installed, then ignore these options.

    a. "MCE_FreqTranslate" :Set for MCE support 
       0:No freq translation, as it is.
       1:Translate the MCE frequency to 6/7/8 freq list

     b. "FixedBandwidth":
     
       0: Normal, as it is set by application
       1: VHF 7MHz , UHF  8MHz 
       6: Fix bandwith as 6MHz 
       7: Fix bandwith as 7MHz 
       8: Fix bandwith as 8MHz 
                                    
    c. "ShiftFreqScan": Skip scan shift frequency (+-167).
        0: Normal, as it is set by application.
        1: Disable off center-frequncy scan (+-167KHz)
 
2. Satellite card setting (DVB-S only)
    a. "DiSEqC" : DiSEqC Selection
        0: None
        1: DiSEqC A
        2: DiSEqC B
        3: DiSEqC C
        4: DiSEqC D
    
    b. "LNBPower" : LNB Power
        0: OFF
        1: ON
    
    c. "Tone" : Tone setting
        0: ON/OFF by LNB switch frequency
        1: OFF
        2: ON

3. Misc setting
    a. "RelockMonitor" : This will create thread to check tuner lock status. If
                         the signal is not locked, it will lock again.
        0: Disable
        1: Enable Relock monitor





