========================================================================
       CONSOLE APPLICATION : THDVBS_BDA_Test
========================================================================
This sample program show how to access Twinhan BDA driver's proprietary IOCTL interfaces.
The IOCTL interface is access through KsProperty interface.

This sample program work with only Twinhan's PCI DVB-S FTA and CI cards, including 
VP1020/VP1022/VP1025/VP1030/VP1032.

To test CI function, please register the filter THPsiParser.ax first.