Overview

Include TBarcode and TDBBarcode. Create barcodes for your applications as easy as typing the code. Simply enter the desired characters and select the type. The barcode will be created!

Developers use Barcode like any other VCL component. Extend your applications with barcode technology with this effective and powerful component.

Barcode supports popular barcodes including Code 39, Code 39 Extended, Code 128, EAN 128, EAN-13, EAN-8, Code 25 Industrial, Code 25 Interleaved, Code 25 matrix, Codabar, UPC-A, UPC-E, UPC+2, UPC+5, Code 93, Code 93 Extended, MSI and Postnet.

Features

- All windows fonts can be used for the optional text, it's Fore- and background colors can be changed free.
- Fore- and background colors of barcode can be changed free.
- Visual in design time.
- Scaleable and rotatlable barcodes and option text.
- All popular barcode types are supported.
- Verification digits are automatically calculated and added for most barcodes.
- Allows Draw the barcode to a canvas (with Scaleable and rotatlable).
- Allows print the barcode to paper (with Scaleable and rotatlable).
- Very popular barcode component software.

Installation (source included)

Delphi 5.x - 7.x

Uninstall previous or evaluation version of Barcode from Delphi IDE. Remove or copy to other directory files of old version to prevent crossing old and new version of Barcode (Including BarcodeDx.bpl, BarcodeDx.dcp files).

Create directory from which you will install Barcode library ('Barcode directory') (for example, C:\Delphi[X]\Barcode).

Copy files from the Barcode archive to 'Barcode directory'.

Use "File\Open..." menu item of Delphi IDE to open the package BarcodeDx.dpk, In "Package..." window click "Compile" button to compile the package and then click "Install" button to register Barcode components on the component palette.

Add, (if needed) 'Barcode directory' in Tools->Environment Options->Library-> Library Path.

Barcode components have to appear on 'Han-soft' page of components palette.

C++Builder 5.x - 6.x

Uninstall previous or evaluation version of Barcode from C++Builder IDE. Remove or copy to other directory files of old version to prevent crossing old and new version of Barcode (Including BarcodeBx.bpl, BarcodeBx.tds files in C++Builder<Install Directory>\Projects\Bpl, and BarcodeBx.lib, BarcodeBx.bpi in C++Builder<Install Directory>\Projects\Lib).

Create directory from which you will install Barcode library ('Barcode directory') (for example, C:\CBuilder[X]\Barcode).

Copy files from the Barcode archive to 'Barcode directory'.

Use "File\Open..." menu item of C++Builder IDE to open the package BarcodeBx.bpk, In "Package..." window click "Compile" button to compile the package.

Add, (if needed) 'Barcode directory' in Tools->Environment Options->Library-> Library Path.

Barcode components have to appear on 'Han-soft' page of components palette.

Installation (trial or without source)

Delphi 5.x - 7.x

Uninstall previous or evaluation version of Barcode from Delphi IDE. Remove or copy to other directory files of old version to prevent crossing old and new version of Barcode (Including BarcodeDx.bpl, BarcodeDx.dcp files).

Create directory from which you will install Barcode library ('Barcode directory') (for example, C:\Delphi[X]\Barcode).

Copy files from the Barcode archive to 'Barcode directory'.

Open "Component\Install packages..." menu item of Delphi IDE, then clicl "Add" Button to add BarcodeDx.bpl in 'Barcode directory'.

Add, (if needed) 'Barcode directory' in Tools->Environment Options->Library-> Library Path.

Barcode components have to appear on 'Han-soft' page of components palette.

C++Builder 5.x - 6.x

Uninstall previous or evaluation version of Barcode from C++Builder IDE. Remove or copy to other directory files of old version to prevent crossing old and new version of Barcode
(Including BarcodeBx.bpl, BarcodeBx.tds files in C++Builder<Install Directory>\Projects\Bpl, and BarcoedBx.lib, BarcodeBx.bpi in C++Builder<Install Directory>\Projects\Lib).

Create directory from which you will install Barcode library ('Barcode directory') (for example, C:\CBuilder[X]\Barcode).

Copy files from the Barcode archive to 'Barcode directory'.

Open "Component\Install packages..." menu item of Delphi IDE, then click "Add" Button to add BarcodeBx.bpl in 'Barcode directory'.

Add, (if needed) 'Barcode directory' in Tools->Environment Options->Library-> Library Path.

Copy 'BarcodeBx.bpl' and 'BarcodeBx.tds'to C++Builder <Install directory>\Projects\Bpl.

Copy 'BarcodeBx.bpi' and 'BarcodeBx.lib'to C++Builder <Install directory>\Projects\Lib.

Barcode components have to appear on 'Han-soft' page of components palette.

Registering and Prices

The Barcode is a Shareware product. If you find it useful and want to receive the latest versions please register your evaluation copy.

Barcode - without source: $79
Barcode - source included: $189
Barcode - source included: $369

You can read detail information about registration at http://www.han-soft.com/purc.php

After registration you will receive (e-mail only) address of registered version for downloading and password for unpacking.

By registering the components you get the following advantages:

1. You will be notified about new versions of the library.
2. You will receive new versions of Barcode FREE till version 3.0.
3. You encourage the author do make the components even better.

About Us

Contact us if you have any questions, comments or suggestions:
Programmer : Han-soft software
Home page : http://www.han-soft.com/
E-mail : support@han-soft.com

Type Define

TUnits = (utMillimeter,utInch);
TOrientation = (toLeftRight, toRightLeft, toTopBottom, toBottomTop);
TCheckSum = (csNone, csModulo10);
TTextShow = (tsNone, tsBarCode, tsBarType, tsBoth);
TTextPosition = (tpTopLeft, tpTopRight, tpTopCenter, tpBottomLeft, tpBottomRight, tpBottomCenter);

TBarType =
(
bcCode_2_5_interleaved,
bcCode_2_5_industrial,
bcCode_2_5_matrix,
bcCode39,
bcCode39Extended,
bcCode128A,
bcCode128B,
bcCode128C,
bcCode93,
bcCode93Extended,
bcCodeMSI,
bcCodePostNet,
bcCodeCodabar,
bcCodeEAN8,
bcCodeEAN13,
bcCodeUPC_A,
bcCodeUPC_E0,
bcCodeUPC_E1,
bcCodeUPC_Supp2,
bcCodeUPC_Supp5,
bcCodeEAN128A,
bcCodeEAN128B,
bcCodeEAN128C
);

Properties

Property | Type | Descriptions
BarType | TBarType | Contains the type of the barcode(bcCode39, bcCode39Extended, bcCode128A, bcCode128B,etc, See also the Type Define)
BarCode | string | Contains the barcode number (or text), general without check digit
BarHeight | Integer | Height of Barcode in Pixels
ColorBar | TColor | Sets the foreground color of the barcode. Black is default
ColorSpc | TColor | Sets the background color of the barcode. White is default
HMargin | Integer | Left and right margin when auto width
CheckSum | TCheckSum | Enable or disable checksum auto-calculation and Algorithms of checksum (csNone, csModulo10)
Modul | Integer | Width of the smallest line in the barcode.
Ratio | Double | Ratio between a wide and a narrow line in a barcode. Normal Values are from 2.0 to 3.0 .
Alignment | TAlignment | Controls the horizontal placement of the barcode within the barcode component(taLeftJustify,taRightJustify,taCenter)
AutWidth | Boolean | Auto adjust component width by barcode width and HMargin (pixels)
Orientation | TOrientation | Orientation of barcode(toLeftRight, toRightLeft, toTopBottom, toBottomTop)
TextShow | TTextShow | Content of barcode line text to display (tsNone, tsBarCode, tsBarType, tsBoth)
TextColor | TColor | Background color of text line
TextPosition | TTextPosition | Position of text line(tpTopLeft, tpTopRight, tpTopCenter, tpBottomLeft, tpBottomRight, tpBottomCenter)
Font | TFont | You can specify the font by name, color, style, effects and the size for the text line
BarTypeName | string | Name of barcode type (read only)
BarWidth | Integer | Width of barcode in pixels (read only)
DataSource | TDataSource | Link the DBBarcode control to a dataset in which the data can be found(Only TDBBarcode)
DataField | String | Use DataField to bind the DBBarcode control to a field in the dataset(Only TDBBarcode)
ReadOnly | Boolean | Set ReadOnly to true to prevent the user from changing the contents of the database field(Only TDBBarcode)
Field | TField | Read Field to get direct access to the contents and properties of the database field without going through the DBBarcode control's Barcode property(Only TDBBarcode)
Color | TColor | See also the help of TPanel in Delphi help.
Align | TAlign
Anchors | TAnchors
BevelInner | TPanelBevel
BevelOuter | TPanelBevel
BevelWidth | Integer
BorderStyle | TBorderStyle
BorderWidth | TBorderWidth
Ctl3D | Boolean
Constraints | TConstraints
Enabled | Boolean
Left | Integer
Height | Integer
Top | Integer
Visual | Boolean
Other properties | See the also help of TPanel in Delphi help.

Methods

Methods | Descriptions
Assign | The Assign method copies all properties from a barcode component to another
Parameters | Source: TPersistent | Source barcode component
Paint | he Paint method is called automatically when a barcode needs update its display area
AutoSetWidth | Auto adjust component width by barcode width and HMargin (pixels)
Parameters | H_Margin: Integer | Left and right margin between barcode and component border (pixels)
Return | Integer | Component width after autowidth (pixels)
Draw | Draw the current barcode to a canvas (with rotate angle)
Parameters | DCanvas:TCanvas | Canvas for draw
const DLeft:Integer | Left margin with Canvas (pixels)
const DTop:Integer | Top margin with Canvas (pixels)
const DHeight:Integer | Height of barcode (pixele)
const DAngle:Double | Angle of left rotate (degree)
Draw | Draw the current barcode to a canvas (current orientation)
Parameters | DCanvas:TCanvas | Canvas for draw
const DLeft:Integer | Left margin with Canvas (pixels)
const DTop:Integer | Top margin with Canvas (pixels)
const DHeight:Integer | Height of barcode (pixels)
GetBarWidth | Get current barcode width
Return | Integer | Barcode width (pixels)
GetBarHeight | Get current barcode height
Return | Integer | Barcode height (pixels)
GetCanvasHeight | Get canvas height of current barcode (with rotate angle)
Parameters | const DHeight:Integer | Height of barcode (pixels)
const DAngle:Double | Angle of left rotate (degree)
Integer | Canvas height of current barcode with rotate angle (pixels)
GetCanvasHeight | Get canvas height of current barcode (current orientation)
Parameters | const DHeight:Integer | Height of barcode (pixels)
Return | Integer | Canvas height of current barcode
GetCanvasWidth | Get canvas width of current barcode (with rotate angle)
Parameters | const DHeight:Integer | Height of barcode (pixels)
const DAngle:Double | Angle of left rotate (degree)
Return | Integer | Canvas width of current barcode with rotate angle (pixels)
GetCanvasWidth | Get canvas width of current barcode (current orientation)
Parameters | const DHeight:Integer | Height of barcode (pixels)
Return | Integer | Canvas width of current barcode (pixels)
Print * | Print current barcode (with rotate angle)
Parameters | const DUnit:TUnits | Unit of length and width(utMillimeter,utInch)
const DLeft:Double | Left margin with paper (mm/inch)
const DTop:Double | Top margin with paper (mm/inch)
const DHeight:Double | Barcode height (mm/inch)
const DModul:Double | Width of thin bar (mm/inch)
const DAngle:Double | Angle of left rotate (degree)
Print * | Print current barcode (current orientation)
Parameters | const DUnit:TUnits | Unit of length and width(utMillimeter,utInch)
const DLeft:Double | Left margin with paper (mm/inch)
const DTop:Double | Top margin with paper (mm/inch)
const DHeight:Double | Barcode height (mm/inch)
const DModul:Double | Width of thin bar (mm/inch)
GetPrnBarWidth | Get barcode width to print
Parameters | const DUnit:TUnits | Unit of length and width(utMillimeter,utInch)
const DModul:Double | Width of thin bar (mm/inch)
Return | Double | Print barcode width (mm/inch)
GetPrnCanvasHeight | Get canvas height of current barcode (with rotate angle)
Parameters | const DUnit:TUnits | Unit of length and width(utMillimeter,utInch)
const DHeight:Double | Barcode height (mm/inch)
const DModul:Double | Width of thin bar (mm/inch)
const DAngle:Double | Angle of left rotate (degree)
Return | Double | Canvas height of current barcode to print (mm/inch)
GetPrnCanvasWidth | Get canvas width of current barcode (with rotate angle)
Parameters | const DUnit:TUnits | Unit of length and width(utMillimeter,utInch)
const DHeight:Double | Barcode height (mm/inch)
const DModul:Double | Width of thin bar (mm/inch)
const DAngle:Double | Angle of left rotate (degree)
Return | Double | Canvas width of current barcode to print (mm/inch)
GetPrnCanvasHeight | Get canvas height of current barcode (current orientation)
Parameters | const DUnit:TUnits | Unit of length and width(utMillimeter,utInch)
const DHeight:Double | Barcode height (mm/inch)
const DModul:Double | Width of thin bar (mm/inch)
Return | Double | Canvas height of current barcode to print (mm/inch)
GetPrnCanvasWidth | Get canvas width of current barcode (current orientation)
Parameters | const DUnit:TUnits | Unit of length and width(utMillimeter,utInch)
const DHeight:Double | Barcode height (mm/inch)
const DModul:Double | Width of thin bar (mm/inch)
Return | Double | Canvas width of current barcode to print (mm/inch)
H_DrawBar | Draw a barcode on canvas
Parameters | H_Canvas:TCanvas | Canvas
const H_BarType:TBarType | Barcode type(bcCode39, bcCode39Extended, bcCode128A, bcCode128B,etc, See also the Type Define)
const H_BarCode:string | Barcode value
const H_Modul:Integer | Width of thin bar (pixels)
const H_Ratio:Double | Ratio of thick and thin bar
const H_CheckSum:TCheckSum | Algorithms of checksum(csNone, csModulo10)
const H_Left:Integer | Left margin with form (pixels)
const H_Top:Integer | Top margin with form (pixels)
const H_Height:Integer | Barcode height (pixels)
const H_TextFont:TFont | Font of brcode text to display
const H_TextShow:TTextShow | Content of barcode text to display(tsNone, tsBarCode, tsBarType, tsBoth)
const H_TextPosition:TTextPosition | Position of barcode text(tpTopLeft, tpTopRight, tpTopCenter, tpBottomLeft, tpBottomRight, tpBottomCenter)
const H_BarColor:TColor; | Color of bar
const H_SpcColor:TColor; | Background Color of barcode
const H_BackColor:TColor; | Background Color of barcode text
const H_Angle:Double | Angle of left rotate (degree)
H_GetBarWidth | Get barcode width to display (pixels)
Parameters | const BW_BarType:TBarType | Barcode type(bcCode39, bcCode39Extended, bcCode128A, bcCode128B,etc, See also the Type Define)
const BW_BarCode:string | Barcode value
const BW_Modul:Integer | Width of thin bar (pixels)
const BW_Ratio:Double | Ratio of thick and thin bar
const BW_CheckSum:TCheckSum | Algorithms of checksum(csNone, csModulo10)
Return | Integer | Barcode width (pixels)
H_GetCanvasWidth | Get canvas width to display (pixels)
Parameters | const CW_BarType:TBarType | Barcode type(bcCode39, bcCode39Extended, bcCode128A, bcCode128B,etc, See also the Type Define)
const CW_BarCode:string | Barcode value
const CW_Modul:Integer | Width of thin bar (pixels)
const CW_Ratio:Double | Ratio of thick and thin bar
const CW_CheckSum:TCheckSum | Algorithms of checksum(csNone, csModulo10)
const CW_Height:Integer | Barcode height (pixels)
const CW_Angle:Double | Angle of left rotate (degree)
Return | Integer | Canvas width to display (pixels)
H_GetCanvasHeight | Get canvas width to display (pixels)
Parameters | const CH_BarType:TBarType | Barcode type(bcCode39, bcCode39Extended, bcCode128A, bcCode128B,etc, See also the Type Define)
const CH_BarCode:string | Barcode value
const CH_Modul:Integer | Width of thin bar (pixels)
const CH_Ratio:Double | Ratio of thick and thin bar
const CH_CheckSum:TCheckSum | Algorithms of checksum(csNone, csModulo10)
const CH_Height:Integer | Barcode height (pixels)
const CH_Angle:Double | Angle of left rotate (degree)
Return | Integer | Canvas width to display (pixels)
H_PrintBar * | Print barcode
Parameters | const H_Unit:TUnits | Unit of width and Height (utMillimeter,utInch)
const H_BarType:TBarType | Barcode type(bcCode39, bcCode39Extended, bcCode128A, bcCode128B,etc, See also the Type Define)
const H_BarCode:string | Barcode value
const H_Modul:Double | Width of thin bar (mm/inch)
const H_Ratio:Double | Ratio of thick and thin bar
const H_CheckSum:TCheckSum | Algorithms of checksum(csNone, csModulo10)
const H_Left:Double | Left margin with form (mm/inch)
const H_Top:Double | Top margin with form (mm/inch)
const H_Height:Double | Barcode height (mm/inch)
const H_TextFont:TFont | Font of brcode text to display
const H_TextShow:TTextShow | Content of barcode text to display(tsNone, tsBarCode, tsBarType, tsBoth)
const H_TextPosition:TTextPosition | Position of barcode text(tpTopLeft, tpTopRight, tpTopCenter, tpBottomLeft, tpBottomRight, tpBottomCenter)
const H_BarColor:TColor; | Color of bar
const H_SpcColor:TColor; | Background Color of barcode
const H_BackColor:TColor; | Background Color of barcode text
const H_Angle:Double | Angle of left rotate (degree)
H_GetPrnBarWidth | Get barcode width to print (mm/inch)
Parameters | const BW_Unit:TUnits | Unit of width and Height(utMillimeter,utInch)
const BW_BarType:TBarType | Barcode type(bcCode39, bcCode39Extended, bcCode128A, bcCode128B,etc, See also the Type Define)
const BW_BarCode:string | Barcode value
const BW_Modul:Double | Width of thin bar (mm/inch)
const BW_Ratio:Double | Ratio of thick and thin bar
const BW_CheckSum:TCheckSum | Algorithms of checksum(csNone, csModulo10)
Return | Double | barcode width (mm/inch)
H_PrnCanvasWidth |  | Get canvas width to print (mm/inch)
Parameters | const CW_Unit:TUnits | Unit of width and Height(utMillimeter,utInch)
const CW_BarType:TBarType | Barcode type(bcCode39, bcCode39Extended, bcCode128A, bcCode128B,etc, See also the Type Define)
const CW_BarCode:string | Barcode value
const CW_Modul:Double | Width of thin bar (mm/inch)
const CW_Ratio:Double | Ratio of thick and thin bar
const CW_CheckSum:TCheckSum | Algorithms of checksum(csNone, csModulo10)
const CW_Height:Double | Barcode height (mm/inch)
const CW_Angle:Double | Angle of left rotate (degree)
Return | Double | canvas width (mm/inch)
H_PrnCanvasHeight | Get canvas height to print (mm/inch)
Parameters | const CH_Unit:TUnits | Unit of width and Height(utMillimeter,utInch)
const CH_BarType:TBarType | Barcode type(bcCode39, bcCode39Extended, bcCode128A, bcCode128B,etc, See also the Type Define)
const CH_BarCode:string | Barcode value
const CH_Modul:Double | Width of thin bar (mm/inch)
const CH_Ratio:Double | Ratio of thick and thin bar
const CH_CheckSum:TCheckSum | Algorithms of checksum(csNone, csModulo10)
const CH_Height:Double | Barcode height (mm/inch)
const CH_Angle:Double | Angle of left rotate (degree)
Return | Double | canvas height (mm/inch)
H_GetBarTypeName | Get barcode type name
Parameters | BN_BarType:TBarType | Barcode type
Return | string | Barcode type name

* Note:Please use the H_PrintBar and Print methods between printer.BeginDoc and printer.EndDoc .
Events

Events | Descriptions
OnChange | Occurs when the barcode, bartype, etc. for the BarCode control may have changed.
Other Events | See also the help of TPanel in <Delphi Help>.