This driver supports the Rancho Tech. RT1600-5 SCSI.


To install Windows NT using this adapter:

1--Copy all files from this directory to a blank formatted floppy in drive A:.
2--Label this disk "RT SETUP"
3--Boot the computer with the Boot Floppy included with Windows NT.
4--Press ENTER to install Windows NT.
5--Select Custom Setup.  Please read your Windows NT manual on Custom Setup.
6--After Windows NT scans for SCSI adapters, press "S" to add an adapter.
7--Select "Other (requires disk provided by hardware manufacturer)".
8--Insert the disk labeled "RT SETUP" into drive A: and press ENTER.
9--Follow the normal Custom Setup installation procedure.


To add support for these drives to an existing Windows NT installation:
1--Copy all files from this directory to a blank formatted floppy in drive A:.
2--Label this disk "RT SETUP"
3--Run the Windows NT SETUP application.
4--Select "ADD/REMOVE SCSI adapters" from the "OPTIONS" menu.
5--Click on the "ADD" button.
6--Select the option "Other (requires a disk from a hardware manufacturer)".
7--Insert the "RT SETUP" disk into drive A: and press ENTER.
8--Select the driver option provided, and press ENTER.
9--Select "Install" and then "Continue".
10-Select "Close", and exit setup.  You will need to restart Windows NT.


Additional Notes:

This driver is not supported for use with Scanners.  