AdapterId 06A14h


AdapterName "NCR WaveLAN Adapter"


NumBytes 4

NamedItem

Prompt "I/O Address Range"

Choice "0400h-07FFh"  pos[3]=xx000001b  io 0400h-07FFh
Choice "0800h-0BFFh"  pos[3]=xx000000b  io 0800h-0BFFh
Choice "0C00h-0FFFh"  pos[3]=xx000000b  io 0C00h-0FFFh
Choice "1000h-13FFh"  pos[3]=xx000000b  io 1000h-13FFh
Choice "1400h-17FFh"  pos[3]=xx000000b  io 1400h-17FFh
Choice "1800h-1BFFh"  pos[3]=xx000000b  io 1800h-1BFFh
Choice "1C00h-1FFFh"  pos[3]=xx000000b  io 1C00h-1FFFh
Choice "2000h-23FFh"  pos[3]=xx000000b  io 2000h-23FFh
Choice "2400h-27FFh"  pos[3]=xx000000b  io 2400h-27FFh
Choice "2800h-2BFFh"  pos[3]=xx000000b  io 2800h-2BFFh
Choice "2C00h-2FFFh"  pos[3]=xx000000b  io 2C00h-2FFFh
Choice "3000h-33FFh"  pos[3]=xx000000b  io 3000h-33FFh
Choice "3400h-37FFh"  pos[3]=xx000000b  io 3400h-37FFh
Choice "3800h-3BFFh"  pos[3]=xx000000b  io 3800h-3BFFh
Choice "3C00h-3FFFh"  pos[3]=xx000000b  io 3C00h-3FFFh
Choice "4000h-43FFh"  pos[3]=xx000000b  io 4000h-43FFh


Help

"16 possible I/O addresses are supported by the WaveLAN adapter.
Conflicting assignments are marked with an asterisk and must be changed."


NamedItem

Prompt  "ROM Address Range :"

Choice  "No ROM Present " pos[0]= xxx1111xb

Help

"Option not available"

NamedItem

Prompt	"Interrupt Select :"
  
choice " Channel 10 " pos[1]=00000000b INT 10
choice " Channel 11 " pos[1]=00000001b INT 11
choice " Channel 12 " pos[1]=00000010b INT 12
choice " Channel 15 " pos[1]=00000011b INT 15
choice " Channel  3 " pos[1]=00000100b INT  3
choice " Channel  5 " pos[1]=00000101b INT  5


Help

"Determines the interrupt level used by the WaveLAN adapter."


