<        CID and Warp Server for e-business - WSeb






















        April 7, 2000





        OS/2 Fix Distribution
        Network Computing Software
        Austin, Tx





        (c) Copyright International Business Machines Corporation, 1997.
        All rights Reserved.

                 April 7, 2000 - Warp Server for e-business CID




                      April 7, 2000 - Warp Server for e-business CID

   CONTENTS


     1.0 Installing WSeb FixPaks via CID   . . . . . . . . . . . . . . . . 1
     1.1  CID Server Setup   . . . . . . . . . . . . . . . . . . . . . . . 1
     1.2  Create a Response File   . . . . . . . . . . . . . . . . . . . . 1
     1.3 Executing FSERVICE  . . . . . . . . . . . . . . . . . . . . . . . 2
       1.3.1 The /T: Parameter   . . . . . . . . . . . . . . . . . . . . . 3
     1.4 Whether to Run SEMAINT  . . . . . . . . . . . . . . . . . . . . . 3
     1.5 Removing an Installed FixPak  . . . . . . . . . . . . . . . . . . 4
     1.6 Some Troubleshooting  . . . . . . . . . . . . . . . . . . . . . . 4
     1.7 Using NvDM/2 and LCU  . . . . . . . . . . . . . . . . . . . . . . 5
     1.8 SERVICE/FSERVICE Differences  . . . . . . . . . . . . . . . . . . 6








































                                                                Contents  ii

                 April 7, 2000 - Warp Server for e-business CID

   FIGURES

     Figure 1. RESPONSE.FIL for Installing WSeb FixPak   . . . . . . . . . 1
     Figure 2. FSERVICE Parameters   . . . . . . . . . . . . . . . . . . . 2
     Figure 3. Invoking FSERVICE   . . . . . . . . . . . . . . . . . . . . 3
     Figure 4. NvDM/2 Profile Example  . . . . . . . . . . . . . . . . . . 5
     Figure 5. LCU REXX Example  . . . . . . . . . . . . . . . . . . . . . 6














































                                                                Figures  iii

                 April 7, 2000 - Warp Server for e-business CID

   1.0 INSTALLING FIXPAKS VIA CID

   Kicker diskettes are required for installing WSeb FixPaks and LAN Server
   (LS) Customer Service Diskettes (which are called FixPaks here). This
   includes installing these FixPaks via IBM's Configuration Installation
   Distribution (CID) process.

   This README assumes that you can do a standard manual installation of a
   FixPak on your system, before you set up a complex CID installation and
   then find that the FixPak does not work on your system.

   The installation kicker diskettes are different from the FixPak data
   diskettes. The same kicker diskettes can be used to install several
   different FixPaks, including all current WSeb and LAN Server FixPaks, and
   certain other products such as DCAF and NetView.

   The following information describes how to use these kicker diskettes to
   install the FixPaks.



   1.1  CID SERVER SETUP

   ž  On the CID server, create a new directory for the FixPak. Here, let's
      name the directory FIXPAK.
   ž  Use the XCOPY command with the /S parameter to copy all of the FixPak
      data diskettes (for either WSeb or LAN Server) into the FIXPAK
      directory.
   ž  XCOPY the single LS kicker diskette into the FIXPAK directory.  (You
      can XCOPY the second WSeb FixPak kicker diskette into the FIXPAK
      directory if you do not have the LS kicker diskette.)




   1.2  CREATE A RESPONSE FILE

   ž  To install an WSeb FixPak, create an FSERVICE response file, using the
      contents of RESPONSE.FIL in the FIXPAKS directory as the basis (see
      Figure 1).

   ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
   :LOGFILE \OS2\INSTALL\SERVICE.LOG
   :FLAGS REPLACE_PROTECTED REPLACE_NEWER
   :SOURCE A:\
   :SERVICE
   :SYSLEVEL \OS2\INSTALL\SYSLEVEL.OS2
   :ARCHIVE \ARCHIVE

   Figure 1. RESPONSE.FIL for Installing WSeb FixPak
   ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ


                                               Installing FixPaks via CID  1

                 April 7, 2000 - Warp Server for e-business CID

   When modifying RESPONSE.FIL, be very careful not to resequence any of the
   statements. Incorrect sequencing is a common cause of problems.

   To service a product that resides in a specific partition, the response
   file keyword :SYSLEVEL is used. For example,

      :SYSLEVEL D:\OS2\INSTALL\SYSLEVEL.OS2


   will only service the WSeb product that already resides in the D:
   partition.

   There is no need to change the :SOURCE statement, because the /S:
   command-line parameter used for the FSERVICE invocation overrides the
   :SOURCE keyword in the response file. Also, the /L1: command-line
   parameter overrides the :LOGFILE keyword.

   It is okay to remove or remark out the :LOGFILE statement, but the
   :SOURCE statement must always be present, even if it is not used.

   The default WSeb response file does not assign drive letters to :SYSLEVEL
   and :ARCHIVE.  This will cause the FSERVICE exec to search all partitions
   to locate the WSeb product, and update all partitions where it finds a
   version of WSeb that is the correct version for the FixPak.  If you
   remove the parameter from :SYSLEVEL then FSERVICE will service all
   products found in the FixPak on all partitions where the products exist.



   1.3 EXECUTING FSERVICE

   ž  Execute FSERVICE to install the FixPak. Figure 2 lists the parameters
      that can be used.

   ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
   /S:   the source path pointing to the FIXPAKS directory on the CID
             server.
   /R:   drive:\path\filename of the response file
   /L1:  drive:\path\filename of the log file
   /T:   (optional) drive:\path to be used if booted from the SEMAINT
             environment; should be set to the same parameter value used in
             the SEMAINT call
   /CID  (optional) to be used for unattended installation
   /SF:  do not use for CID install

   Figure 2. FSERVICE Parameters
   ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ

   Figure 3 on page 3 gives an example of invoking the FSERVICE exec.
   Depending on what the response file contains, the call in Figure 3 on
   page 3 could be used to install a FixPak, back out a FixPak, or commit a


                                               Installing FixPaks via CID  2

                 April 7, 2000 - Warp Server for e-business CID

   FixPak (so that the FixPak cannot be backed out once it is installed).
   All code in Figure 3 must be on a single command line.

   ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
   x:\csd\fixpak\fservice
     /s:x:\csd\fixpak
     /r:x:\csd\fixpak\response.fil
     /cid /t:c:\service
     /l1:x:\log\fixpak\service.log

   Figure 3. Invoking FSERVICE
   ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ




   1.3.1 THE /T: PARAMETER

   If you boot WSeb from a hard drive and the environment variable
   REMOTE_INSTALL_STATE is set to 0 or 1, you must use the /T: parameter.
   If you boot from a hard drive and the REMOTE_INSTALL_STATE environment
   variable is not defined, you should not use the /T: parameter. If you
   boot from diskette, /T: is ignored.

   FSERVICE uses the /T: parameter to decide whether a file should be
   updated. If the first part of the path to a file is equal to the /T:
   parameter, then FSERVICE will not update that file, because files in the
   maintenance directory (created by SEMAINT) should not be updated.



   1.4 WHETHER TO RUN SEMAINT

   The best and safest way to install an WSeb FixPak is in a maintenance
   mode. You can install an WSeb FixPak while booted in normal WSeb PM mode,
   but problems may occur. If you install the FixPak while in the WSeb PM
   mode you must reboot the system as soon as possible after the FixPak
   install completes. If you install two FixPaks in a row then reboot the
   system the locked file device driver will not work correctly.

   There are two standard ways to enter maintenance mode -- you can use
   SEMAINT to generate a maintenance boot environment, or you can boot from
   diskette. If you are going to install several fixes at one time, using
   SEMAINT will save time because it requires fewer reboots and no
   processing of locked files.

   To use SEMAINT, you must make changes to the way you invoke FSERVICE.
   FSERVICE cleans up a maintenance directory created by SEMAINT if the /T:
   parameter is used and the system is booted from a hard drive.




                                               Installing FixPaks via CID  3

                 April 7, 2000 - Warp Server for e-business CID

   You should only use the /T: parameter in the first FSERVICE call you
   make. You need to remove or not use the /T: parameter in all other calls
   to FSERVICE. This is necessary because the /T: parameter may cause a file
   that was already updated to be restored to the original level.

   If you use SEMAINT, do not use the /S2: parameter.



   1.5 REMOVING AN INSTALLED FIXPAK

   To back out a FixPak that has already been installed, use the response
   file shown below.

      :LOGFILE C:\OS2\INSTALL\SERVICE.LOG
      :TARGET ARCHIVE
      :BACKOUT
      :SYSLEVEL C:\OS2\INSTALL\SYSLEVEL.OS2


   When backing out a FixPak, the FSERVICE parameter /S: should point to the
   FIXPAK directory on the CID server, because FSERVICE needs to find the
   product information files for the FixPak that it will back out.



   1.6 SOME TROUBLESHOOTING

   If problems occur during a FixPak installation, it may be necessary to
   delete or rename the LOGF0000.??? and the LOGFSTART.??? files from the
   target client system and to remove the ARCHIVE directory. These steps are
   frequently needed when a previous FixPak installation started but failed
   to finish.

   The current WSeb FixPak boot diskettes are based on OS/2 Warp code. The
   system can be booted from either OS/2 3 or OS/2 Warp 4 to install the
   FixPak.

   When installing a FixPak for LS 4.0 or some other product, you may need
   to change the response file keyword <code> :SYSLEVEL <end code> to point
   to the correct SYSLEVEL.??? file for that product.

   You may need to remove or remark out the response file keyword :ARCHIVE
   if archiving is turned off for the FixPak. This is the case for many LS
   FixPaks.



                                               Installing FixPaks via CID  4

                 April 7, 2000 - Warp Server for e-business CID

   You can archive to a LAN drive. You can archive files for different
   products to the same directory.

   You must always use the same archive directory for the same product. If
   you install an OS/2 FixPak and a previous OS/2 FixPak was installed on
   the system, you must use the same archive directory as used before. You
   can change the archive directory with a special response file keyword,
   :REDIRECT.

   To update several products, you may need several pairs of :SERVICE and
   :SYSLEVEL parameters for each product.



   1.7 USING NVDM/2 AND LCU

   Users of NetView Distribution Manager for OS/2 (NvDM/2), IBM's premier
   CID process, should refer to Figure 4 for a sample profile. For users of
   LAN CID Utility (LCU), the standard CID process, see the REXX command
   file product definition example in Figure 5 on page 6.

   ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
   TargetDir = "C:\SERVICE"
   CompNameLen = 4

   Section Catalog
   Begin
     ObjectType = SOFTWARE
     GlobalName = FIXPAK.WARP.17.C.REF.1.0
     Description = WARP FixPak 17 on C:
   End

   Section Install
   Begin
     Program = SA:\IMG\FIXW17\FSERVICE.EXE
     Parms = "/S:$(SourceDir) /T:$(TargetDir)
       /R:$(SA)\IMG\FIXW17\SERVICEC.RSP /L1:$(Logfile1)"
     SourceDir =  SA:\IMG\FIXW17
     LogFile1 = SB:\LOGS\OS2\$(WorkStatName).FIX
   End

   Figure 4. NvDM/2 Profile Example
   ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ










                                               Installing FixPaks via CID  5

                 April 7, 2000 - Warp Server for e-business CID

   ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ

   x.fixpak = 9
   x.9.name='WARP FixPak 17'
   x.9.statevar = 'CAS_' || x.9.name
   x.9.instprog = 'x:\img\fixw17\fservice.exe ',
                  '/S:x:\img\fixw17 ',
                  '/L1:y:\logs\os2\' || client || '.fix ',
                  '/CID ',
                  '/R:'
   x.9.rspdir = 'x:\img\fixw17'
   x.9.default = 'response.fil'

   Figure 5. LCU REXX Example
   ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ




   1.8 SERVICE/FSERVICE DIFFERENCES

   The Fixtool utility SERVICE will not work from a LAN drive.  This is
   working as designed. SERVICE will only work from "removable" media such
   as floppy diskette and CDROM.  FSERVICE is designed to work from floppy
   diskette, CDROM, hard drive, LAN drive, etc.




























                                               Installing FixPaks via CID  6
