<        Installation instructions for Warp Server for e-business FixPak
        XRGE001















        

        
        



        May 26, 2000

        This FixPak makes the products it services Year 2000 ready
        
        Build level 14.040
        
        This FixPak applies to:
        
        CSD Level:    XRG4500    Warp Server for e-business (UNI)
        Component ID: 5639A6150
        Version:      4.50
        Type:         0S
        
        CSD Level:    XRG4500    Warp Server for e-business (SMP)
        Component ID: 5639A5550
        Version:      4.50
        Type:         0S
        
        Requires Corrective Service Facility release f.142 or later
        
        OS/2 Fix Distribution
        Personal System Products
        Austin, Tx
        
        
        (c) Copyright International Business Machines Corporation, 1981, 1998.
        All rights Reserved.

        May 26, 2000 - Warp Server for e-business FixPak XRGE001




         May 26, 2000 - Warp Server for e-business FixPak XRGE001

   CONTENTS


     1.0 Terms and Conditions  . . . . . . . . . . . . . . . . . . . . . . 1

     2.0 Do not use your system  . . . . . . . . . . . . . . . . . . . . . 2

     3.0 Installation Notes  . . . . . . . . . . . . . . . . . . . . . . . 3

     4.0 Platform Specific Drivers (PSDs)  . . . . . . . . . . . . . . . . 4
       4.0.1 Please use Fixtool f.142 or later   . . . . . . . . . . . . . 6
       4.0.2 Using Display Recovery Choices  . . . . . . . . . . . . . . . 6
       4.0.3 No products found   . . . . . . . . . . . . . . . . . . . . . 6
       4.0.4 Previous installation interrupted   . . . . . . . . . . . . . 7
       4.0.5 Unable to open Archive directory  . . . . . . . . . . . . . . 7
       4.0.6 CSF0208 No products were found on the target ...    . . . . . 8
       4.0.7 CSF0249 Error opening or creating archive file.   . . . . . . 8
       4.0.8 Printer installation process change   . . . . . . . . . . . . 8
       4.0.9 Configuration Installation Distribution ( CID )   . . . . . . 8

     5.0 Post Installation Notes   . . . . . . . . . . . . . . . . . . . . 9

     6.0 New Function   . . . . . . . . . . . . . . . . . . . . . . . . . 10
     6.1 Intel"s new SpeedStep  . . . . . . . . . . . . . . . . . . . . . 10
     6.2 New RAS Utilities added  . . . . . . . . . . . . . . . . . . . . 10
     6.3 JFS lazywrite parameters on the IFS= line in config.sys  . . . . 10
     6.4 Graphics Adapter Device Drivers (GRADD)  . . . . . . . . . . . . 11
     6.5 REXX New Function  . . . . . . . . . . . . . . . . . . . . . . . 11
     6.6 Other README files   . . . . . . . . . . . . . . . . . . . . . . 12

     7.0 Corrective Service Facility  . . . . . . . . . . . . . . . . . . 13
       7.0.1 Required CSF level   . . . . . . . . . . . . . . . . . . . . 13
       7.0.2 Where you can find CSF code  . . . . . . . . . . . . . . . . 13
       7.0.3 Creating FixPak diskettes  . . . . . . . . . . . . . . . . . 14
     7.1 Read-Only files  . . . . . . . . . . . . . . . . . . . . . . . . 14
     7.2 SYSLEVEL file locations  . . . . . . . . . . . . . . . . . . . . 15
     7.3 Relocated Warp Server for e-business file support  . . . . . . . 15

     8.0 Installation Process   . . . . . . . . . . . . . . . . . . . . . 17
     8.1 Before installation  . . . . . . . . . . . . . . . . . . . . . . 17
     8.2 Method 1: Install from booted OS/2 partition.    . . . . . . . . 17
     8.3 Method 2: Install from alternate bootable media  . . . . . . . . 18
     8.4 Additional Corrective Service Facility information   . . . . . . 19

     9.0 CSD level of SYSLEVEL.OS2  . . . . . . . . . . . . . . . . . . . 20
       9.0.1 FixPak Syslevel File   . . . . . . . . . . . . . . . . . . . 20

     10.0 FixPak Corrective Service levels and disk layouts   . . . . . . 21

     11.0 Space Utilization   . . . . . . . . . . . . . . . . . . . . . . 28
       11.0.1 Recovering FixPak ARCHIVE and BACKUP space  . . . . . . . . 28

   
                                                                Contents  ii


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

       11.0.2 TRADEMARKS  . . . . . . . . . . . . . . . . . . . . . . . . 29



















































   
                                                               Contents  iii


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   1.0 TERMS AND CONDITIONS

   Important - please read the following terms and conditions.

   Downloading the Service Fixes included in FixPak XRGE001 for Warp Server
   for e-business indicates your acceptance of the following terms and
   conditions:

   1. You must be, and agree that you are, a current licensee of Warp Server
      for e-business.
   2. You may make copies of the Warp Server for e-business Service Fixes
      equal to the number of licensed copies of Warp Server for e-business
      you possess.
   3. You may only use the Warp Server for e-business Service Fixes included
      with FixPak XRGE001 for maintenance purposes.
   4. All other terms and conditions of your Warp Server for e-business
      license agreements apply to the Service Fixes; however, this does not
      extend any warranty and/or services, including but not limited to the
      "Initial Installation" period, outlined in such agreements.

































   
                                                     Terms and Conditions  1


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   2.0 DO NOT USE YOUR SYSTEM

   Once you begin a FixPak installation, do not try to use your system for
   any other purpose. Doing so may yield unexpected problems which can cause
   the FixPak installation to fail.















































   
                                                   Do not use your system  2


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   3.0 INSTALLATION NOTES



















































   
                                                       Installation Notes  3


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   4.0 PLATFORM SPECIFIC DRIVERS (PSDS)

   In Warp Server for e-business SMP, we have removed all the platform
   specific code from the operating system, and placed it into platform
   specific drivers.  These drivers provide an abstraction layer for the
   underlying hardware by allowing the OS to call generic functions to
   perform platform specific operations without worrying about the actual
   hardware implementation.  This allows us to support new platforms without
   modifying the operating system.

   PSD's are specified in CONFIG.SYS by using the PSD keyword, and must
   conform to the 8.3 file naming convention (e.g. PSD=BELIZE.PSD). They
   cannot contain either drive, or path information because OS/2 cannot
   process such information at the stage of the startup sequence when the
   PSD statements are processed.  The root directory of the startup
   partition is first searched for the specified file name, then the \OS2
   directory of the startup partition. If drive or path information is
   included in a PSD statement, an error is generated.

   PSD parameters may be specified after the PSD's name, and may be a
   maximum of 1024 characters long. The parameter string is not interpreted,
   or parsed by OS/2, it is passed verbatim, as an ASCIIZ string when the
   PSD's Install function is invoked.

   If multiple PSD statements are encountered. OS/2 will load each PSD in
   the order listed in CONFIG.SYS, and call the PSD's install function. The
   first PSD which successfully installs, will be the one OS/2 uses.

   PSD statements are processed before BASEDEV, IFS, and DEVICE statements.

   Please note that any time you add or make changes to the CONFIG.SYS file,
   you must restart the system in order for the changes to become effective.
   The CONFIG.SYS file is read only during system startup. Anything added to
   this file after system initialization does not work until you restart the
   system.

   This PSD has the following syntax for its argument line:

   [/apic] [/p=<n>] [/nmi=[l]int<n>] [/pic=[l]int<n>] [/prec=<pstr>]

   Where:
    /apic   indicates that the PSD should enable symetric interrupt
            mode.

    /p      indicates that the system should be configured for <n>
            processors where <n> is a decimal number (ie 5, 8, 12).

    /nmi    indicates to the system a default signal route for NMIs.
            This allows the route to be specified for NMIs if there
            isn't one defined by the MP configuration tables set up
            by BIOS.

   
                                         Platform Specific Drivers (PSDs)  4


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

            By using the /prec option (see below), it is possible to
            override what is in the MP configuration tables in the
            event that they have been built incorrectly by the BIOS.

            The argument is "int<n>" or "lint<n>".  The first case
            indicates the interrupt pin number to which the NMI signal
            is wired on the I/O apic.  The second case indicates the
            interrupt poin number to which the NMI signal is wired on
            the local apic.  <n> is a decimal number (ie 0, 3, 12).

    /pic    indicates to the system a default signal route for the
            8259 interrupt controller when the system is running in
            "virtual wire" mode.  This allows the route to be specified
            for the interrupt controller if there isn't one defined by
            the MP configuration tables set up by BIOS.  By using the
            /prec option (see below), it is possbile to override what is
            in the MP configuration tables in the event that they have
            been built incorrectly by the BIOS.

    /prec   indicates to the system the precedence order to be used in
            determining the routing for the NMI signal and the
            interrupt signal from the interrupt controller.  This
            allows control over the choosing of a routing entry when
            there is more than one entry.

            There are three (3) possible entries that can describe a
            route:
                    route to the I/O APIC
                    route to the Local APIC
                    route described by argument(s) to the PSD

            The first two may be specified in the MP configuration tables
            that are built by the BIOS.  The third may be specified on the
            argument line to the PSD.

            Each type of route is described by one letter.  "i" for the
            I/O APIC routes, "l" for the local APIC routes, and "d" for
            the routes described by the argument line to the PSD.

            The precedence string is *exactly* 3 characters long.  The
            first character indicates the type of routes to be considered
            first, the second indicates the routes to be considered next
            and the third indicates the routes that are to be considered
            last.

            As an example, "ild" indicates that I/O APIC routes are to
            considered first, followed by local APIC routes and finally
            routes specified on the argument line.  In contrast, "dil"
            indicates that routes on the argument line are to be considered
            first, then the I/O APIC and finally the local APIC.


   
                                         Platform Specific Drivers (PSDs)  5


           May 26, 2000 - Warp Server for e-business FixPak XRGE001


   Note: The arguments to the PSD are NOT case sensitive.


   4.0.1 PLEASE USE FIXTOOL F.142 OR LATER

   For Warp Server for e-business FixPak 01, you must use Corrective Service
   Facility f.142 or later.

   If you try to use a CSF level prior to f.142 you may get a "CSF0208 No
   products were found on the target system to service" message.


   4.0.2 USING DISPLAY RECOVERY CHOICES

   If you have the "Display Recovery Choices at each system startup"
   function active on your system, you need to disable it before you apply a
   FixPak if

   þ  The system is running
   þ  The boot partition will be serviced.

   The problem with using this function is that the Corrective Service
   Facility (CSF) updates the current CONFIG.SYS with entries to run the
   Locked File Device Driver (LFDD) the next time you boot the system. This
   is done to replace files that are currently in use (locked) by the
   system.

   The Recovery choices function replaces the current CONFIG.SYS with the
   one that is associated with the recovery choice you select, wiping out
   the LFDD entries. This means the LFDD does not run at boot time and the
   deferred files will not get updated, therefore the FixPak does not get
   completely applied.

   Note: It is not necessary to disable this function if you install a
   FixPak by booting from the CSF disks or from another OS/2 partition.


   4.0.3 NO PRODUCTS FOUND

   If you see a "No products were found on the target system to service"
   message while applying this FixPak, there is probably a mismatch between
   the data in \OS2\INSTALL\SYSLEVEL.OS2 and what is supported by this
   FixPak.

   Compare the data for the Warp Server for e-business Base Operating System
   from the SYSLEVEL command output with the same values listed at the end
   of this document in the "FixPak Corrective Service levels and disk
   layouts" section.  They must be identical.



   
                                         Platform Specific Drivers (PSDs)  6


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   If these values are correct, check for the following files on any OS/2
   boot drive in the \OS2\INSTALL directory.

      LOGF0000.OS2
      LOGSTART.OS2
      LOGARCH.OS2


   Check for the following files in your MMOS2\INSTALL directory.

      LOGF0000.MPM
      LOGSTART.MPM
      LOGARCH.MPM


   Also check for the following file:

      C:\CSF_SEL.000


   If these files exist, rename them and try the FixPak installation again.
   Delete the renamed files after the FixPak has been applied.


   4.0.4 PREVIOUS INSTALLATION INTERRUPTED

   If you get a message that the previous installation of a FixPak was
   interrupted (whether true or not), check for the following files and
   directory on all drives:

     Files:
        FIXSTART
        IBMCSFLK.LST
        IBMCSFLK.CSF
        CSF_*

     Directory:
        IBMCSFLK


   If any exist, rename them and try the FixPak installation again.  Delete
   the renamed files after the FixPak has been applied.


   4.0.5 UNABLE TO OPEN ARCHIVE DIRECTORY

   If you get a message about problems with the Archive directory (for
   example, cannot find or unable to open), then the most probable cause is
   that you applied a previous FixPak and have since deleted the FixPak
   ARCHIVE or BACKUP directory.


   
                                         Platform Specific Drivers (PSDs)  7


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   To recover from this, follow the "No files to service" and "Previous
   installation interrupted" steps listed above.


   4.0.6 CSF0208 NO PRODUCTS WERE FOUND ON THE TARGET ...

   This means no SYSLEVEL files was found that had a CSD Level, COMPID,
   Version and Type that matched any of the SYSLEVEL files supported by this
   FixPak. Run the SYSLEVEL command and record the output for SYSLEVEL.OS2
   in the OS2/INSTALL directory on your boot drive. Compare this data with
   the data contained in the README.1ST file on FixPak disk 1.

   To recover from this, rename the existing SYSLEVEL.OS2 file to SYSL.OS2
   and copy SYSLEVEL.OS2 from your Warp Server for e-business found on
   installation DISK 1.


   4.0.7 CSF0249 ERROR OPENING OR CREATING ARCHIVE FILE.

   Typically this means the FixPak Archive directory has been deleted but
   the files that point to it still exist. You need to delete the
   LOGF000.OS2 and LOGSTART.OS2 files from your OS2/INSTALL directory.
   LOGSTART.OS2 has the R/O attribute set and it needs to be reset before
   the file can be deleted.  There may also be a LOGARCH.OS2 file that needs
   to be deleted.

   This can also occur for Multi Media Presentation Manager/2 (MMPM). You
   would then need to delete the LOGF0000.MPM and LOGSTART.MPM files from
   the \MMOS2\INSTALL directory and possibly LOGARCH.MPM if it exists.


   4.0.8 PRINTER INSTALLATION PROCESS CHANGE

   If you install a new printer by clicking MB2 on the Printer icon in the
   templates folder then clicking on Install, the printer object will now be
   created in the Printer folder, not on the Desktop.


   4.0.9 CONFIGURATION INSTALLATION DISTRIBUTION ( CID )

   Read the README.CID on Disk # 1 for an example of how to set up a
   response file to do a CID install.










   
                                         Platform Specific Drivers (PSDs)  8


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   5.0 POST INSTALLATION NOTES



















































   
                                                  Post Installation Notes  9


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   6.0 NEW FUNCTION

   It is our policy not to include new function in FixPaks. However, as with
   any policy there may be exceptions. If any exception occurs in the
   future, we will communicate them to you in this section of the
   README.1ST.


   6.1 INTEL"S NEW SPEEDSTEP

   The support for Intel's new SpeedStep (a.k.a. Geyserville) is NOT
   included in this FixPak. It will be made available where you downloaded
   this FixPak from in a separate ZIP file.


   6.2 NEW RAS UTILITIES ADDED

   Two new RAS utilities are included for Pak 01: PSFILES.EXE and
   PSSEMS.EXE.

   PSFILES.EXE can dump out information about open files on the system.  By
   default, it dumps out the information for all processes. Alternately,
   "PSFILES xxx" will dump out information for PID xxx (xxx is a hex number,
   e.g. from PSTAT).

   PSSEMS.EXE can dump out information about open 32 bit semaphores on the
   system By default it prints out all the shared (i.e. system-wide)
   semaphores.  Usage is:  pssems [/n] [hex_pid | /a] ; where /n suppresses
   shared semaphores and /a prints pruivate sems for all system processes.

   Note: These RAS Utilities are added to the OS2 directory on your system.


   6.3 JFS LAZYWRITE PARAMETERS ON THE IFS= LINE IN CONFIG.SYS

       IFS=jfs.ifs /L:OFF
       IFS=jfs.ifs /L:synctime,maxage,bufferidle


   (JFS ignores any characters between the L (or l) and the colon, so valid
   flags are /L: /LAZY: /LW: /lazywrite: etc.)

   OFF forces asynchonous writes to be immediately initiated.

   synctime is the interval at which the sync thread runs. Default = 64

   maxage is the longest time that a frequently modified file is kept in
   cache
           default = synctime*4

   bufferidle is the time indicating a "recent" change.  Changes newer than

   
                                                            New Function  10


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

           this value are not written unless the last write was older than
           maxage.  default = MIN(1,synctime/8)

   (All parameters in seconds)

        IFS=C:\OS2\JFS.IFS /L:64

        synctime = 32, maxage = 128, bufferidle = 4

        IFS=C:\OS2\JFS.IFS /LW:10,60,5

        synctime = 10, maxage = 60, bufferidle = 5

        IFS=C:\OS2\JFS.IFS /LAZYWRITE:4,60

        synctime = 4, maxage = 60, bufferidle = 1

        IFS=C:\OS2\JFS.IFS /lazy:off

        All writes initiated immediately (synctime=1, maxage=bufferidle=0)
        Note: sync thread still runs since trivial things like marking an
        inode accessed are still deferred.


   The cachejfs.exe command allows the lazywrite parameters to be changed
   immediately.  The syntax is to the IFS line, except that the /L: prefix
   is optional.  In addition, the cachejfs command can modify the minimum
   and maximum number of free cache buffers to be maintained.  Calling
   cachejfs with no parameters reports the current settings.

   CACHEJFS [[/LAZYWRITE:]{OFF|syncTime[,maxAge[,bufferIdle]]}]
   /MINFREE:minfree
            /MAXFREE:maxfree


   6.4 GRAPHICS ADAPTER DEVICE DRIVERS (GRADD)

   Future updates for GRADD and other video drivers (when they are released)
   will be found via the internet at:

   þ  http://service.software.ibm.com/pslaunch.html



   6.5 REXX NEW FUNCTION

   New Function has been added in REXX. Please see the "Other README Files"
   for documentation pointers. This new function was added to FP 1 and
   later.



   
                                                            New Function  11


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   6.6 OTHER README FILES

   There are other README files containing information you may want to
   review.  All README files are found on the first FixPak disk and are not
   copied to your system when the Fixpak is installed.

   File           Use

   README2        Problems fixed in each FixPak (APAR list)

   README.CID     Installing FixPaks via CID

   README.DBG     Description of Debug files for Warp Server for e-business
                  debugging.

   READREXX.TXT   New RexxUtil Function documentation added in this FixPak.




































   
                                                            New Function  12


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   7.0 CORRECTIVE SERVICE FACILITY



   7.0.1 REQUIRED CSF LEVEL

   You should use release level f.142 or later of the OS/2 Corrective
   Service Facility to install this FixPak.

   Bootable diskettes are no longer provided starting with the F.138B CSF
   build. Instead, you now get a self-extracting ZIP file which contains the
   following:

      archctl.cmd
      build.lvl
      csfpans.dll
      filefix.dll
      fpinst.cmd
      fservice.exe
      fservice.msg
      ibmcsflk.dll
      ibmcsflk.exe
      ibmcsflk.msg
      ibmcsflk.sys
      msg.dll
      nls.dll
      pack.exe
      read.me
      readme.inf
      response.lan
      response.wp3
      response.wp4
      service.exe
      service.hlp
      shpiinst.dll
      unpack.exe
      unpack2.exe
      viocalls.dll


   Follow the directions in the READ.ME file to use the new CSF code. It
   covers the use of SERVICE.EXE and FSERVICE.EXE from a booted partition or
   from one of several alternative boot methods.


   7.0.2 WHERE YOU CAN FIND CSF CODE

   The Corrective Service Facility code is available from many places,
   including, but not limited to, the following:

   Source         How to access

   
                                             Corrective Service Facility  13


           May 26, 2000 - Warp Server for e-business FixPak XRGE001


   Internet(FTP)  Anonymous FTP to ftp.software.ibm.com in the
                  "/ps/products/os2/fixtool" directory.

   Internet(WWW)  Point your Web Browser at
                  ftp://service.boulder.ibm.com/ps/products/os2/fixtool

   Intranet(FTP)  Anonymous FTP to os2service.austin.ibm.com in the
                  "f:\fixpacks\fixtool" directory.



   7.0.3 CREATING FIXPAK DISKETTES

   Use LOADDSKF.EXE to create the diskettes. For each disk image, place a
   2MB HD (1.44MB formatted) diskette in A:.

   Warning: DO NOT use a 1MB (720KB formatted) diskette because you might
   have problems trying to install this FixPak.

   For each diskette image in the FixPak, do the following:

   Enter LOADDSKF XRGE001.?DK A: /F  (? can be 1 through 9, A through Z).

   Label the diskette as

         FixPak XRGE001
   Corrective Service Diskette ?
          (CSF DISK ?)


   Note: For diskette images ADK through ZDK, use the numbers 10 through 35.

        Examples:

        XRGE001.ADK = 10
        XRGE001.FDK = 15
        XRGE001.LDK = 21
      etc.




   7.1 READ-ONLY FILES

   Some files being updated by this FixPak may have the Read-Only attribute
   set. If you are using the A:SERVICE method to install this FixPak you
   will be asked if you want the files replaced.

   Press the "OK" button.


   
                                             Corrective Service Facility  14


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   7.2 SYSLEVEL FILE LOCATIONS

   This FixPak will service directories based on the location of a supported
   SYSLEVEL.OS2 file.  Please check your system to make sure extra copies of
   this file are not located in directories other than:

     \OS2\INSTALL\SYSLEVEL.OS2 on the boot drive of your OS/2 partition(s)


   If additional copies of these files are found in other locations on your
   hard disk then CSF will try to service files as follows:

   For \OS2\INSTALL\SYSLEVEL.OS2

     ..\..\           all files in a directory two levels above (toward the
                      root). This should be the root directory of your boot
                      drive.

     ..\*             all files in a directory one level above (toward the root)
                      and all subdirectories below. This should be the OS2
                      directory and subdirectories.

     ..\..\VT\*       all files in the VT directory and subdirectories.

     ..\..\PSFONTS\*  all files in the PSFONTS directory and subdirectories.

     ..\..\LANGUAGE\* all files in the LANGUAGE directory and subdirectories.

     ..\..\OPENDOC\*  all files in the OPENDOC directory and subdirectories.




   7.3 RELOCATED WARP SERVER FOR E-BUSINESS FILE SUPPORT

   If you have moved Warp Server for e-business files or directories to a
   drive other than the one the SYSLEVEL.OS2 file is on, do the following in
   order to have them serviced:

   þ  Create a file named USERDIRS.OS2 in the \OS2\INSTALL directory of the
      Warp Server for e-business partition to be serviced.

      In this file, place the full path to the directories you want to be
      serviced. Assuming your boot drive is C: and you installed Multimedia
      on the D: drive and manually moved WINOS2 support to the E: drive:







   
                                             Corrective Service Facility  15


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

       D:\MMOS2
       D:\MMOS2\DLL
       D:\MMOS2\DSP
       D:\MMOS2\HELP
       D:\MMOS2\IMAGES
       D:\MMOS2\INETTEMP
       D:\MMOS2\INSTALL
       D:\MMOS2\MACROS
       D:\MMOS2\MOVIES
       D:\MMOS2\SOUNDS
       D:\MMOS2\SOUNDS\DESKTOP
       D:\MMOS2\SOUNDS\GARDEN
       D:\MMOS2\SOUNDS\OCEAN
       D:\MMOS2\SOUNDS\SPACE
       E:\OS2\MDOS\WINOS2
       E:\OS2\MDOS\WINOS2\SYSTEM
       E:\OS2\MDOS\WINOS2\TEMP


   Note: Leave this file for any future Warp Server for e-business FixPaks
   you might apply. The easy way to create this file is to use the DIR
   command with the /A:D /S /B parameters and pipe the output to a file.

      dir d:\mmos2 /a:d /s /b > anyfile


   Then copy that data into the USERDIRS.OS2 file.

   With CSF release level F.142 or later, you can use wildcards, so your
   USERDIRS.OS2 file would be much simpler and would look like:

       D:\MMOS2\*
       E:\OS2\MDOS\WINOS2\*



















   
                                             Corrective Service Facility  16


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   8.0 INSTALLATION PROCESS



   8.1 BEFORE INSTALLATION

   Before installing any FixPak, run CHKDSK /F against all drives on your
   system to correct any file system errors that might be present. You
   cannot do this while OS/2 is active. You must shut down and run CHKDSK by
   one of the following methods:

   þ  Boot from your Installation, DISK 1 and DISK 2 diskettes.  If your
      file system is HPFS, then put the diskette with CHKDSK and UHPFS.DLL
      on it in your A: drive before issuing the CHKDSK command.
   þ  Boot from the Utilities disk you created via the "Create Utility
      Diskettes" icon in the System Setup folder.
   þ  Boot from a different OS/2 partition.

   Once CHKDSK has completed, reboot your system then shutdown all running
   applications before starting the FixPak installation.


   8.2 METHOD 1: INSTALL FROM BOOTED OS/2 PARTITION.

   Note: CS_???.EXE below means CS_142 or later.

   Follow the instructions in the READ.ME file that comes in the CS_???.EXE
   self-extracting zip file.  This explains how to use the CS_???.EXE file
   and the various ways you can install a FixPak with this level of CSF
   code.

   Here are some additional notes:

   Follow the displayed instructions.  When prompted to insert Corrective
   Service Diskette 1 (not CSF DISK Diskette 1), place FixPak XRGE001
   Corrective Service Diskette 1 in drive A. Repeat for the rest of the
   FixPak disks when requested to do so.

   It can take a considerable length of time for the Corrective Service
   Facility to scan your hard disk for serviceable files.  In some cases, it
   has taken as long as 40 minutes.  Please be patient and allow this
   process to complete.

   If this is the first OS/2 Warp FixPak you have applied to this system,
   then enter the path to the directory where a copy of replaced files will
   be stored (for example, D:\ARCHIVE or E:\FIXPAK\ARC, etc.)

   Note: This ARCHIVE directory is not related to the ARCHIVES directory
   built into OS/2 Warp 3 and Warp 4. Please specify a different path.  You
   must specify a different ARCHIVE directory for each product to be
   serviced.

   
                                                    Installation Process  17


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   If this is not the first OS/2 Warp FixPak, then enter the path to the
   BACKUP directory where a copy of replaced files will be stored (for
   example, D:\BACKUP).

   Note: You must specify a different BACKUP directory for each product to
   be serviced.

   Make sure there is sufficient space available on the drive you specify
   for archive or backup.  Even though these files are kept in compressed
   (PACK2) format, they can take up a lot of space on the drive.

   During the installation process you may see messages about Archiving,
   Updating and Deferring service.

   þ  Archiving saves a compressed copy of the original file in the ARCHIVE
      or BACKUP path you specified.
   þ  Updating means the original files are replaced with the new ones from
      this FixPak.
   þ  Deferring service means the file to be updated is currently in use by
      the system and cannot be updated.  The new files from the FixPak are
      placed in unpacked format in the \IBMCSFLK\FIX directory on the drive
      with the most free space.  They are processed by the locked file
      device driver during reboot after you shut down the system.

   See the section "FixPak Corrective Service levels and disk layouts" for
   the CSD levels this FixPak applies to.

   You will see the following during reboot of the system if you applied
   service to the OS/2 partition you were booted from.

      The locked file driver is loaded.

             Processing locked files

             Processing complete


   The system will do one automatic reboot after the Locked File Device
   Driver has completed.


   8.3 METHOD 2: INSTALL FROM ALTERNATE BOOTABLE MEDIA

   Note: CS_???.EXE below means CS_142 or later.

   Follow the instructions in the READ.ME file that comes in the CS_???.EXE
   self-extracting zip file.  This explains how to use the CS_???.EXE file
   and the various ways you can install a FixPak with this level of CSF
   code.



   
                                                    Installation Process  18


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   Here are some additional notes:

   This method does not prompt the user for any information.  No interaction
   with the user takes place other than requests to put the next diskette in
   drive A. All serviceable partitions on your system will be updated
   automatically unless you have modified the default response file.  Be
   especially careful of extra SYSLEVEL.OS2 or SYSLEVEL.MPM files when using
   this method because they can cause CSF to apply service to directories
   you do not want serviced.

   See the section "FixPak Corrective Service levels and disk layouts" for
   the CSD levels this FixPak applies to.

   Note: It can take a considerable length of time for the Corrective
   Service Facility to scan your hard disk for serviceable files.  Please be
   patient and allow this process to complete.

   Note: You can edit the response file to control some of the actions taken
   by FSERVICE.EXE while applying a FixPak.  See the READ.ME file or use the
   VIEW command to look at the file README.INF.  They are part of
   CS_???.EXE.


   8.4 ADDITIONAL CORRECTIVE SERVICE FACILITY INFORMATION

   Additional information on the Corrective Service Facility, like how to
   backout a FixPak, is available from the README.INF file on the first
   Corrective Service Facility disk.  To view this file, place CSF disk 1 in
   drive A and enter VIEW A:\README.INF.

   There is also some additional information in the READ.ME file.





















   
                                                    Installation Process  19


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   9.0 CSD LEVEL OF SYSLEVEL.OS2

   The Current CSD level field of the SYSLEVEL.OS2 file in each serviced
   partition will be updated with the name of the FixPak when it is applied.

   All fix information is recorded in SERVICE.LOG. Look at the file

      \OS2\INSTALL\SERVICE.LOG


   on your boot drive for information relating to the installation of
   FixPaks on your system.

   Additionally, you can use the VER /R command to see the current revision
   of OS/2 installed.  The response will look like the following for this
   FixPak:

   The Operating System/2 Version is 4.50
   Revision 14.040


   The first page of this document has a line that looks like:

   Build Level: n.nnn


   That is the number you should see for this FixPak when you issue the VER
   /R command.


   9.0.1 FIXPAK SYSLEVEL FILE

   A SYSLEVEL.FPK will be added to the OS2\INSTALL directory when this
   FixPak is installed. It is titled "OS/2 Warp Server for e-business
   Service Level".  It contains the name of the currently installed FixPak
   in both the Current and Previous CSD level fields and is located in the
   same directory the SYSLEVEL.OS2 file is located in which should be
   \OS2\INSTALL.

   The easiest way to look at SYSLEVEL information is to use the SYSLEVEL
   command and redirect the output to a file then edit the file and search
   for SYSLEVEL.FPK.










   
                                               CSD level of SYSLEVEL.OS2  20


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   10.0 FIXPAK CORRECTIVE SERVICE LEVELS AND DISK LAYOUTS

   Build Level: 14.040

   Product location on CSD:  A:\FIX\OS2.1
   Product name:  "Warp Server for e-business Base Operating System (UNI)"
   Standard Edition  4.50
   Fixpak name:   XRGE001_   (Country = Germany)
   Pre-requisite CSD Level:  XRG4500_
   System Id:  1000
   Component Id:  5639A6150
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "Warp Server for e-business Base Operating System (SMP)"
   Standard Edition  4.50
   Fixpak name:   XRGE001_   (Country = Germany)
   Pre-requisite CSD Level:  XRG4500_
   System Id:  1000
   Component Id:  5639A5550
   Archive is ON for this product.
   ________________________________________________________________________

   Default directories:

           ..\*
           ..\..\MMOS2
           ..\..\MMOS2\*
           ..\..\VT
           ..\..\VT\*
           ..\..\TOPOBJ
           ..\..\TOPOBJ\*
           ..\..\PSFONTS
           ..\..\PSFONTS\*
           ..\..\LANGUAGE
           ..\..\LANGUAGE\*
   Will create the following directories
      ..\..\   Stub File:  @ROOTDIR

      ..\..\OS2   Stub File:  @OS2DIR

      ..\..\OS2\DLL   Stub File:  @DLLDIR

      ..\..\OS2\HELP   Stub File:  @HELPDIR

      ..\..\OS2\INSTALL   Stub File:  @INSTDIR

      ..\..\OS2\INSTALL\UNI   Stub File:  @UNIDIR

      ..\..\OS2\INSTALL\SMP   Stub File:  @SMPDIR

      ..\..\OS2\SYSTEM   Stub File:  @SYSTDIR

   
                       FixPak Corrective Service levels and disk layouts  21


           May 26, 2000 - Warp Server for e-business FixPak XRGE001


      ..\..\OS2\PDPSI\PMDF\WARP45_U   Stub File:  @WARP45U

      ..\..\OS2\PDPSI\PMDF\WARP45_S   Stub File:  @WARP45S


   Files contained in Fixpak for product:

   Filename      Name on CSD   Disk#  Date        Time   Size     Checksum
   ------------  ------------  -----  ----------  -----  -------  --------
   ANSI.SYS      ANSI.SY_       10    01/21/2000  17:20     7480  C871A248
   ATTRIB.EXE    ATTRIB.EX_     10    01/21/2000  17:11    37789  BF02FFB9
   CACHE.EXE     CACHE.EX_      10    02/16/2000  18:54    14382  5C4AC774
   CACHEJFS.EXE  CACHEJFS.EX_   10    04/05/2000  09:28    43882  76D0A6BA
   CCHMAIN.EXE   CCHMAIN.EX_     7    04/20/2000  15:14   199344  D2EE798C
   CHKDSK.COM    CHKDSK.CO_      9    01/21/2000  17:12    72768  3B53B220
   CHKDSK.SYS    CHKDSK.SY_     10    02/16/2000  18:55      795  3BAD8348
   CHKDSK32.DLL  CHKDSK32.DL_    8    02/16/2000  19:07   187867  49E7104C
   CHKLGJFS.EXE  CHKLGJFS.EX_    9    04/05/2000  09:41    87435  810817FC
   CLRBBLKS.EXE  CLRBBLKS.EX_    9    04/05/2000  09:27    34974  0805912D
   CMD.EXE       CMD.EX_         8    01/21/2000  17:14   102156  0D8BAA26
   CREX.MSG      CREX.MS_       10    03/27/2000  14:23     2865  87FEDE0E
   CREXUTIL.DLL  CREXUTIL.DL_    9    03/27/2000  14:23    68119  4D4C346B
   CREXX.DLL     CREXX2.DL_      7    03/27/2000  14:23   266031  E0EEAA5F
   DDINSTAL.EXE  DDINSTAL.EX_   10    03/16/2000  09:36    52775  DE448AF4
   DEFRAGFS.EXE  DEFRAGFS.EX_    9    04/05/2000  09:41    33994  A20E887B
   DF_DEB.EXE    DF_DEB.SM_      8    03/31/2000  09:47   145137  4A177D0E
   DF_DEB.EXE    DF_DEB.UN_      8    03/31/2000  11:01   137525  C3224040
   DF_RET.EXE    DF_RET.SM_      8    03/31/2000  09:00   145105  E839266C
   DF_RET.EXE    DF_RET.UN_      8    03/31/2000  08:45   137493  F151EF0D
   DOSCALL1.DLL  DOSCALL1.SM_    7    03/31/2000  11:18   144860  C84ADF21
   DOSCALL1.DLL  DOSCALL1.UN_    7    03/31/2000  11:17   137587  671B4178
   DOSCALL1.SYM  DOSC1SYM.SM_   10    03/31/2000  11:18    43972  80433297
   DOSCALL1.SYM  DOSC1SYM.UN_   10    03/31/2000  11:17    43636  7ADF7845
   DOSKRNL       DOSKRNL.___    10    03/31/2000  11:18    31525  89B813C5
   DSPIMRI.DLL   DSPIMRI.DL_    10    04/11/2000  14:19    26662  11858862
   DSPINSTL.EXE  DSPINSTL.EX_    8    04/13/2000  10:33   174616  9395A9AA
   E.EXE         E.EX_           9    04/20/2000  14:02    63383  6771744D
   EAUTIL.EXE    EAUTIL.EX_     10    01/21/2000  17:16    38512  5BCC93C5
   ENGINE.DLL    ENGINE.DL_     10    04/05/2000  10:55    43330  1B93C994
   ETKE603.DLL   ETKE603.DL_     3    11/23/1999  16:02   863453  FFCC7CD4
   EXTENDFS.EXE  EXTENDFS.EX_   10    04/05/2000  09:41    29304  9C49402F
   FFIPC.DLL     FFIPC.DL_      10    02/15/2000  11:49    34653  AC79EF4B
   FIBASE.RSP    FIBASE.RS_      8    03/17/2000  11:26   984421  96847973
   GRE2VMAN.DLL  GRE2VMAN.DL_   10    04/18/2000  09:40    20653  3414D817
   GSVINST.EXE   GSVINST.EX_     9    03/29/2000  15:41    34351  5CF8E60E
   HELPMGR.DLL   HELPMGR.DL_     6    04/18/2000  10:09   277411  69768510
   HPFS.IFS      HPFS.IF_        8    02/16/2000  18:52   141890  E4DB1086
   HPFS.TDF      HPFS.TD_       10    02/16/2000  18:52     1620  A7A46813
   INSCFG32.DLL  INSCFG32.DL_   10    03/15/2000  14:23    44914  60032F10
   INSTALL.EXE   INSTALL.EX_     6    03/16/2000  09:27   658923  A4962962

   
                       FixPak Corrective Service levels and disk layouts  22


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   JAVA.RSP      JAVA.RS_       10    03/15/2000  11:19   453012  F76673BD
   JFS.IFS       JFS.IF_         7    04/05/2000  14:55   170664  307C8E3E
   JFS.MSG       JFS.MS_        10    04/05/2000  10:56    14942  74A8E9B6
   JFS.TDF       JFS.TD_        10    04/05/2000  14:55    16706  5414E862
   JFSCHK32.EXE  JFSCHK32.EX_   10    04/05/2000  09:27     6493  091534C9
   JFSH.MSG      JFSH.MS_       10    04/05/2000  10:56    10299  673ED200
   KERNEL.SDF    KRNLRSDF.SM_    9    03/31/2000  09:00    59320  A77C0A5A
   KERNEL.SDF    KRNLRSDF.UN_    9    03/31/2000  08:45    58993  74A800C7
   KERNELD.SDF   KRNLDSDF.SM_    9    03/31/2000  09:47    59486  CB7358E8
   KERNELD.SDF   KRNLDSDF.UN_    9    03/31/2000  12:15    59138  6DD281B6
   KEYBOARD.DCP  KEYBOARD.DC_   10    12/02/1999  14:21   315109  639280C8
   LOGDUMP.EXE   LOGDUMP.EX_     8    04/05/2000  09:41    78712  C8B4F97E
   LVM.DLL       LVM.DL_         7    04/05/2000  10:53   148355  844A23BC
   LVM.EXE       LVM.EX_         8    04/05/2000  09:48    92928  794EE0E1
   LVM.MSG       LVM.MS_        10    04/05/2000  10:54    21017  24EC6706
   LVMALERT.EXE  LVMALERT.EX_   10    04/05/2000  09:38    22784  0880C0B5
   LVMGUI.ZIP    LVMGUI.ZI_      8    04/05/2000  10:54   464162  76542B3B
   LVMH.MSG      LVMH.MS_       10    04/05/2000  10:54    21551  0B1AE59A
   NAMEREXX.DLL  NAMEREXX.DL_    8    04/18/2000  09:48    97763  307B5ADD
   OREXUTIL.DLL  ORXUTIL2.DL_    9    03/27/2000  14:23    42823  AA36CA95
   OREXX.DLL     OREXX2.DL_      5    03/27/2000  14:23   490355  38ED06D5
   OS2APIC.PSD   OS2APIC.PS_    10    03/31/2000  09:02    31232  0EE0FB78
   OS2DASD.DMD   OS2DASD.DM_     9    04/05/2000  09:36    37421  78E0D44F
   OS2DUMP       OS2DUMP.___    10    03/31/2000  12:13    15197  13734DDD
   OS2KRNL       OS2KRNL.SM_     3    03/31/2000  08:56   884502  9F649D8C
   OS2KRNL       OS2KRNL.UN_     4    03/31/2000  08:41   824485  20E86D6E
   OS2KRNLB.SYM  KRNLBSYM.SM_    7    03/31/2000  09:57   190388  C3DE2C17
   OS2KRNLB.SYM  KRNLBSYM.UN_    7    03/31/2000  09:35   183300  DD36AD48
   OS2KRNLD.SYM  KRNLDSYM.SM_    2    03/31/2000  09:45   195716  01133A70
   OS2KRNLD.SYM  KRNLDSYM.UN_    7    03/31/2000  09:23   188132  948D711C
   OS2KRNLR.SYM  KRNLRSYM.SM_    8    03/31/2000  08:56   170468  18D778B8
   OS2KRNLR.SYM  KRNLRSYM.UN_    8    03/31/2000  08:41   165924  3DB3CE51
   OS2LDR        OS2LDR.SM_     10    03/31/2000  11:03    43008  755F6A61
   OS2LDR        OS2LDR.UN_     10    03/31/2000  11:02    45056  540AC542
   OS2LVM.DMD    OS2LVM.DM_      9    04/05/2000  09:38    31471  7AAA80B0
   OSO001.MSG    OSO001.MS_      9    02/07/2000  16:21   217070  239D81C0
   OSO001H.MSG   OSO001H.MS_     8    02/07/2000  16:21   293318  8B278E06
   PICV.DLL      PICV.DL_       10    04/18/2000  16:20    29784  B58D633B
   PMCTLS.DLL    PMCTLS.DL_      2    04/19/2000  07:28   644468  E38DD21B
   PMCTLS.SYM    PMCTLSYM.SM_   10    04/19/2000  07:28    44660  BE9B7D52
   PMCTLS.SYM    PMCTLSYM.UN_   10    04/19/2000  07:28    44660  BE9B7D52
   PMDDEML.DLL   PMDDEML.DL_    10    04/18/2000  09:51    28278  F9338E04
   PMGPI.DLL     PMGPI.DL_       1    04/18/2000  09:46   373634  290D3B3A
   PMGPI.TDF     PMGPI.TD_      10    04/18/2000  09:46    12338  9DBC9676
   PMGRE.DLL     PMGRE.DL_      10    04/18/2000  16:05     2231  5B0E2F80
   PMGRE.TDF     PMGRE.TD_      10    04/19/2000  07:29     1062  6A88EB40
   PMMERGE.DLL   PMMERGE.DL_     1    04/19/2000  07:29  1268435  4A73753C
   PMMERGE.SYM   PMMERSYM.SM_    8    04/19/2000  07:29   117492  38CCF139
   PMMERGE.SYM   PMMERSYM.UN_    8    04/19/2000  07:29   117492  38CCF139
   PMREXX.EXE    PMREXX.EX_      9    04/18/2000  09:48    78885  65DBB279
   PMSHAPI.DLL   PMSHAPI.DL_    10    04/18/2000  09:53     4549  DBE5FDDD

   
                       FixPak Corrective Service levels and disk layouts  23


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   PMSHAPI.TDF   PMSHAPI.TD_    10    04/19/2000  07:29     6726  C5BE654A
   PMSPL.DLL     PMSPL.DL_       6    04/20/2000  13:46   393425  040DCAB9
   PMSPL.SYM     PMSPLSYM.SM_   10    04/20/2000  13:46    32340  CBBED451
   PMSPL.SYM     PMSPLSYM.UN_   10    04/20/2000  13:46    32340  CBBED451
   PMVIOP.DLL    PMVIOP.DL_      9    04/18/2000  16:21    65934  8193EDAE
   PMVIOP.SYM    PMVIOSYM.SM_   10    04/18/2000  16:21     7620  FC539948
   PMVIOP.SYM    PMVIOSYM.UN_    5    04/18/2000  16:21     7620  FC539948
   PMWINX.DLL    PMWINX.DL_      5    04/18/2000  16:19   530859  95DC432A
   PMWP.DLL      PMWP.DL_        2    04/21/2000  21:21  1063613  61889D88
   PMWP.SYM      PMWPSYM.SM_     9    04/21/2000  21:21   103780  86296A0F
   PMWP.SYM      PMWPSYM.UN_     9    04/21/2000  21:21   103780  86296A0F
   PMWP.TDF      PMWP.TD_       10    04/21/2000  21:21    13825  D3003BC4
   PMWPMRI.DLL   PMWPMRI.DL_     7    04/20/2000  13:39    57383  FDFF16CA
   PNP.DLL       PNP.DL_        10    04/20/2000  13:51    36297  864E5850
   PNP.SYS       PNP.SY_        10    12/03/1999  07:09     2152  ACA5C755
   PRINTPNP.PND  PRINTPNP.PN_   10    02/24/2000  15:08    14105  587E7543
   PSFILES.EXE   PSFILES.EX_    10    01/21/2000  17:18    10229  D7031046
   PSSEMS.EXE    PSSEMS.EX_     10    01/21/2000  17:18    11717  BE2AAF39
   PSTAT.EXE     PSTAT.EX_      10    01/21/2000  17:17    14661  8322A525
   QUECALLS.DLL  QUECALLS.DL_    7    03/31/2000  12:14     1024  A32F1956
   QUECALLS.TDF  QUECALLS.TD_   10    03/31/2000  08:44     1299  347856DA
   README.CID    README.CI_     10    03/16/2000  09:22    56006  0FE6D00A
   REGEDIT2.EXE  REGEDIT2.EX_    4    11/24/1999  13:35   970240  A92BBDD6
   REX.MSG       REX.MS_        10    03/27/2000  14:23     2865  6D1DD657
   REXX.DLL      CREXX1.DL_      6    03/27/2000  14:23   266031  75D50B8E
   REXX.DLL      OREXX1.DL_      5    03/27/2000  14:23   490355  1A317A06
   REXX.IMG      REXX.IM_        9    03/27/2000  14:23   283636  D7ED399D
   REXXAPI.DLL   REXXAPI.DL_    10    03/27/2000  14:23    40995  2E213324
   REXXC.EXE     REXXC.EX_      10    03/27/2000  14:23     2758  D085D34F
   REXXCRT.DLL   REXXCRT.DL_     9    04/18/2000  09:33    79348  C116A7D8
   REXXUTIL.DLL  REXXUTIL.DL_    9    03/27/2000  14:23    68119  4D50480F
   REXXUTIL.DLL  ORXUTIL1.DL_    9    03/27/2000  14:23    42823  AA514A95
   RINSTPRN.EXE  RINSTPRN.EX_    7    04/20/2000  14:05   209396  BBFD5E94
   RSPDDI.EXE    RSPDDI.EX_      4    03/15/2000  14:40    29753  02E48B4A
   RSPDSPI.EXE   RSPDSPI.EX_     9    04/13/2000  10:33   143398  6EACD6CE
   RSPIMRI.DLL   RSPIMRI.DL_     3    04/11/2000  14:19    26671  401F536B
   RSPINST.EXE   RSPINST.EX_     6    03/16/2000  09:34   476880  C39966DC
   SCENTER.DLL   SCENTER.DL_     6    04/20/2000  14:00   300861  710BB39C
   SEAMLESS.DLL  SEAMLESS.DL_   10    04/19/2000  07:38    49167  4779F519
   SESDD32.SYS   SESDD32.SY_     9    01/04/2000  12:47   118834  8B2CC722
   SESMGR.DLL    SESMGR.DL_     10    03/31/2000  12:14     1536  46610CE5
   SESMGR.TDF    SESMGR.TD_     10    03/31/2000  08:44     1877  941F4208
   SHELL.SDF     SHELLSDF.SM_   10    03/31/2000  09:00    21279  280E0B5C
   SHELL.SDF     SHELLSDF.UN_   10    03/31/2000  09:00    21279  280E0B5C
   SOFTDRAW.DLL  SOFTDRAW.DL_    5    04/18/2000  09:39   467527  96D2B7BA
   SYSLEVEL.EXE  SYSLEVEL.EX_    9    03/16/2000  09:23    44656  3E496C6D
   SYSLEVEL.FPK  SYSLEVEL.FP_    5    01/13/2000  10:25      165  21150A29
   SYSLEVEL.MSG  SYSLEVEL.MS_   10    03/16/2000  09:23     1536  8773B291
   TRACE.EXE     TRACE.EX_      10    01/21/2000  17:28    56064  A1136FC6
   TRAPDUMP.EXE  TRAPDUMP.EX_    9    02/16/2000  05:03    30236  B98D8FF7
   TRC012F.TFF   TRC012F.TF_    10    04/05/2000  14:55    35285  5AFF5E53

   
                       FixPak Corrective Service levels and disk layouts  24


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   TRCUST.EXE    TRCUST.EX_      9    01/21/2000  17:28    98773  00550BBF
   UHPFS.DLL     UHPFS.DL_       9    02/16/2000  19:07   107536  C1FD3396
   UJFS.DLL      UJFS.DL_        3    04/11/2000  14:10   237065  08687C64
   USBAUDIO.SYS  USBAUDIO.SY_   10    12/03/1999  08:34    25332  FC4F64B4
   USBCOM.SYS    USBCOM.SY_     10    12/03/1999  08:34    18294  A18CFE84
   USBD.SYS      USBD.SY_       10    12/15/1999  19:17    18034  60FBC9DB
   USBHID.SYS    USBHID.SY_     10    12/15/1999  19:17    12060  85A9116F
   USBMON.EXE    USBMON.EX_     10    03/29/2000  15:41    20105  ABD22E4F
   USBMOUSE.SYS  USBMOUSE.SY_   10    12/15/1999  19:17    11898  FEDED7D9
   USBPRT.HLP    USBPRT.HL_     10    04/20/2000  14:06     7356  4C07F0E2
   USBPRT.PDR    USBPRT.PD_      9    04/20/2000  14:06    40007  1695D362
   USBUHCD.SYS   USBUHCD.SY_    10    12/03/1999  08:32    23342  7EF549D7
   USBUHCD2.SYS  USBUHCD2.SY_   10    12/03/1999  08:32    23342  1AB19794
   USER.EXE      USER.EX_        6    01/06/2000  13:05   281552  1D4B87AF
   VCU.EXE       VCU.EX_         7    04/05/2000  13:58   130631  238A3BAB
   VCU.MSG       VCU.MS_         6    04/05/2000  10:54     1838  173F9CB7
   VMAN.DLL      VMAN.DL_        9    04/18/2000  09:40    60953  64D19979
   VMANWIN.SYS   VMANWIN.SY_    10    04/11/2000  13:25     3024  91B58399
   VWIN.SYS      VWIN.SY_       10    11/23/1999  11:10    27104  94AA32A6
   WINSCLIP.DLL  WINSCLIP.DL_   10    01/06/2000  12:48    14848  463DF894
   WINSHELD.EXE  WINSHELD.EX_   10    01/06/2000  12:48    22528  E0091276
   WINSMSG.DLL   WINSMSG.DL_     1    01/06/2000  12:48    28441  ED40951E
   WPREXX.IMP    WPREXX.IM_     10    03/27/2000  14:23     6313  8425963F

   ************************************************************************
   Product location on CSD:  A:\FIX\OS2.2
   Product name:  "Warp Server for e-business Base Operating System (UNI)"
   Standard Edition  4.50
   Fixpak name:   XRGE001_   (Country = Germany)
   Pre-requisite CSD Level:  XRG4500_
   System Id:  1000
   Component Id:  5639A6150
   Archive is ON for this product.
   ________________________________________________________________________

   Default directories:

           ..\..\
           ..\..\OS2\dll

   Files contained in Fixpak for product:

   Filename      Name on CSD   Disk#  Date        Time   Size     Checksum
   ------------  ------------  -----  ----------  -----  -------  --------
   DOSCALL1.DLL  DCALLUNI.___   10    03/31/2000  11:17   137587  671B4178
   OS2KRNL       KRNLUNI.___    11    03/31/2000  08:41   824485  20E86D6E
   OS2LDR        LDRUNI.___     10    03/31/2000  11:02    45056  540AC542

   ************************************************************************
   Product location on CSD:  A:\FIX\OS2.3
   Product name:  "Warp Server for e-business Base Operating System (SMP)"

   
                       FixPak Corrective Service levels and disk layouts  25


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   Standard Edition  4.50
   Fixpak name:   XRGE001_   (Country = Germany)
   Pre-requisite CSD Level:  XRG4500_
   System Id:  1000
   Component Id:  5639A5550
   Archive is ON for this product.
   ________________________________________________________________________

   Default directories:

           ..\..\
           ..\..\OS2\dll

   Files contained in Fixpak for product:

   Filename      Name on CSD   Disk#  Date        Time   Size     Checksum
   ------------  ------------  -----  ----------  -----  -------  --------
   DOSCALL1.DLL  DCALLSMP.___   10    03/31/2000  11:18   144860  C8601F21
   OS2KRNL       KRNLSMP.___    12    03/31/2000  08:56   884502  9F649D8C
   OS2LDR        LDRSMP.___     10    03/31/2000  11:03    43008  755F6A61

   ************************************************************************
   Product location on CSD:  A:\FIX\OS2.4
   Product name:  "Warp Server for e-business Base Operating System (UNI)"
   Standard Edition  4.50
   Fixpak name:   XRGE001_   (Country = Germany)
   Pre-requisite CSD Level:  XRG4500_
   System Id:  1000
   Component Id:  5639A6150
   Archive is ON for this product.
   ________________________________________________________________________

   Default directories:

           ..\*
           ..\..\MMOS2
           ..\..\MMOS2\*
           ..\..\VT
           ..\..\VT\*
           ..\..\TOPOBJ
           ..\..\TOPOBJ\*
           ..\..\PSFONTS
           ..\..\PSFONTS\*
           ..\..\LANGUAGE
           ..\..\LANGUAGE\*

   Files contained in Fixpak for product:

   Filename      Name on CSD   Disk#  Date        Time   Size     Checksum
   ------------  ------------  -----  ----------  -----  -------  --------
   PMDF.EXE      PMDF.EX_       10    02/16/2000  05:02   393388  03A72FBC

   
                       FixPak Corrective Service levels and disk layouts  26


           May 26, 2000 - Warp Server for e-business FixPak XRGE001


   ************************************************************************
   Product location on CSD:  A:\FIX\OS2.5
   Product name:  "Warp Server for e-business Base Operating System (SMP)"
   Standard Edition  4.50
   Fixpak name:   XRGE001_   (Country = Germany)
   Pre-requisite CSD Level:  XRG4500_
   System Id:  1000
   Component Id:  5639A5550
   Archive is ON for this product.
   ________________________________________________________________________

   Default directories:

           ..\*
           ..\..\MMOS2
           ..\..\MMOS2\*
           ..\..\VT
           ..\..\VT\*
           ..\..\TOPOBJ
           ..\..\TOPOBJ\*
           ..\..\PSFONTS
           ..\..\PSFONTS\*
           ..\..\LANGUAGE
           ..\..\LANGUAGE\*

   Files contained in Fixpak for product:

   Filename      Name on CSD   Disk#  Date        Time   Size     Checksum
   ------------  ------------  -----  ----------  -----  -------  --------
   PMDF.EXE      PMDF.EX_       11    02/15/2000  11:51   390792  A8C1A335





















   
                       FixPak Corrective Service levels and disk layouts  27


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   11.0 SPACE UTILIZATION

   The FixPak installation process requires free space on the following
   drives:

   Space needed   Drive
   Up to 2MB      C:
   Up to 2MB      Boot drive (4MB if boot is C:)
   Up to 22MB     Drive with most free space, holds deferred files if
                  A:SERVICE method used.
   Up to 26MB     FixPak Archive/Backup for product with CSD level of
                  XRG4500

   Note: The lines labeled "FixPak Archive/Backup for product with CSD level
   of" will be on the drive you specify and will occupy up to the size
   indicated for the Archive and for the Backup directories. If, for
   example, the indicated size is 30MB then the space actually occupied on
   the drive can be up to 60MB.


   11.0.1 RECOVERING FIXPAK ARCHIVE AND BACKUP SPACE

   Warning: Make sure you read and understand the following before removing
   the Archive and Backup files and directories.

   You can recover the space used for FixPak Archive and Backup files as
   long as you understand that doing this prevents you from being able to
   backout to the previous Backup or Archive level. If it becomes necessary
   at a later time to backout a FixPak, the only way you can do this is to
   reinstall Warp.

   Do the following to delete the FixPak Backup and Archive files and remove
   the files used by CSF to keep track of what service has been applied to
   your system.

   1.  Delete every instance of the following files on your system
       (search every drive and every directory they contain).
       þ   LOGF0000.*   (can be OS2 or MPM)
       þ   LOGSTART.*   (can be OS2 or MPM)
       þ   LOGARCH.*    (can be OS2 or MPM)
       þ   CSF_*.*
       þ   FIXSTART
   2.  Delete the files in the FixPak Archive and Backup directories on
       your harddisk.
   3.  Remove the FixPak Archive and Backup directories with the RMDIR
       command.






   
                                                       Space Utilization  28


           May 26, 2000 - Warp Server for e-business FixPak XRGE001

   11.0.2 TRADEMARKS

   The following terms are trademarks of the International Business Machines
   Corporation in the United States or other countries or both:

   þ  IBM
   þ  OS/2
   þ  WorkSpace On-Demand

   Other company, product, and service names may be trademarks or service
   marks of others.









































   
                                                       Space Utilization  29
