      SID

        COMMANDS

            Command              Meaning

         As              (Assemble)    Enter assembly language
                                       statements
                                       s is the start address

         Cs{b{,d}}       (Call)        Call to memory location from SID
                                       s is the called address
                                       b is the value of the BC register
                                       pair d is the value of the DE
                                       register pair

         D{W}{s}{,f}     (Display)     Display memory in hex and ASCII
                                       W is a 16-bit word format
                                       s is the start address
                                       f is the finish address

         Epgm-filespec   (Load)        Load program and symbol table
          {,sym-filespec}              for execution

         E*sym-filespec  (Load)        Load a symbol table file

         Fs,f,d          (Fill)        Fill memory with constant value
                                       s is the start address
                                       f is the finish address
                                       d is an eight-bit data item

         G{p}{,a{,b}}     (Go)         Begin Execution
                                       p is a start address
                                       a is a temporary breakpoint

         H                (Hex)        Displays all symbols with
                                       addresses in Hex
         H.a                           Displays hex, decimal, and ASCII
                                       values of a where
                                       a is a symbolic expression

         Ha,b                          Computes hex sum and difference
                                       of a and b where
                                       a and b are symbolic expressions

         Icommand tail   (Input)       Input CCP command line

         L{s}{,f}        (List)        List 8080 mnemonic instructions
                                       s is the start address
                                       f is the finish address

         Ms,h,d          (Move)        Move Memory Block
                                       s is the start address
                                       h is the high address of the block
                                       d is the destination start address

         P{p{,c}}        (Pass)        Pass point set, reset, and display
                                       p is a permanent breakpoint address
                                       c is initial value of pass counter

         Q               (Quit)        Exit SID (for compatibility with
                                       80x86 versions of SID)

         Rfilespec{,d}   (Read)        Read Code/Symbols
                                       d is an offset to each address

         S{W}s           (Set)         Set Memory Values
                                       s is address where value is sent
                                       W is 16 bit word

         T{n{,c}}        (Trace)       Trace Program Execution
                                       n is the number of program steps
                                       c is the utility entry address.

         T{W}{n{,c}}     (Trace)       Trace Without Call
                                       W instructs SID not to trace
                                       subroutines
                                       n is the number of program steps
                                       c is the utility entry address

         U{W}{n{,c}}     (Untrace)     Monitor Execution without Trace
                                       n is the number of program steps
                                       c is the utility entry address
                                       W instructs SID not to trace
                                       subroutines

         V                (Value)      Display the value of the next
                                       available location in memory
                                       (NEXT), the next location after
                                       the largest file read in (MSZE),
                                       the current value of the Program
                                       counter (PC), and the address of
                                       the end of available memory (END)

         Wfilespec,s,f  (Write)        Write the contents of a contiguous
                                       block of memory to filespec.
                                       f is finish address

         X{f}{r}        (Examine)      Examine/alter CPU state.
                                       f is flag bit C,Z,M,E or I.
                                       r is register A,B,D,H,S or P.

    HELP>