      DEVICE

        EXAMPLES

      A>DEVICE

           Displays the physical devices and   current  assignments  of
           the logical devices in the system.

      A>DEVICE NAMES

           Lists the physical devices with a   summary  of  the  device
           characteristics.

      A>DEVICE VALUES

           Displays  the  current  logical  device assignments.

      A>DEVICE CRT

           Displays the attributes  of  the  physical device CRT.

      A>DEVICE CON

           Displays the  assignment  of  the  logical device CON:

      A>DEVICE CONOUT:=LPT,CRT

           Assigns  the  system   console    output  (CONOUT:)  to  the
           printer (LPT) and the screen (CRT).

      A>DEVICE AUXIN:=CRT2 [XON,9600]

           Assigns the auxiliary logical input   device   (AUXIN:)   to
           the   physical   device   CRT   using  protocol XON/XOFF and
           sets the transmission rate for the device  at  9600.

      A>DEVICE LST:=NULL

           Disconnects the list output logical device (LST:).

      A>DEVICE LPT [XON,9600]

           Sets  the  XON/XOFF  protocol  for  the physical device  LPT
           and sets the transmission speed at 9600.

      A>DEVICE CONSOLE [PAGE]

           Displays the current console  page  width  in  columns   and
           length in lines.

      A>DEVICE CONSOLE [COLUMNS=40 LINES=16]

           Sets the screen size to 40 columns and 16 lines.

    HELP>