      LINK

        OPTIONS

      Use LINK option switches to control  execution parameters.   Link
      options    follow    the    file  specifications and are enclosed
      within square  brackets.   Multiple  switches  are  separated  by
      commas.

                                 LINK-80 Options

              A          Additional memory; reduces buffer space
                         and writes temporary data to disk

              B          BIOS link in banked CP/M 3 system.
                         1.  Aligns data segment on page boundary.
                         2.  Puts length of code segment in header.
                         3.  Defaults to .SPR filetype.

              Dhhhh      Data origin; sets memory origin for
                         common and data area

              Gn         Go; set start address to label n

              Lhhhh      Load; change default load address
                         of module to hhhh.   Default 0100H

              Mhhhh      Memory size; Define free memory
                         requirements for MP/M modules.

              NL         No listing of symbol table at console

              NR         No symbol table file

              OC         Output .COM command file.  Default

              OP         Output .PRL page relocatable file for
                         execution under MP/M in relocatable
                         segment

              OR         Output .RSP resident system process file
                         for execution under MP/M

              OS         Output .SPR system page relocatable file
                         for execution under MP/M

              Phhhh      Program origin; changes default
                         program origin address to hhhh.
                         Default is 0100H.

              Q          Lists symbols with leading question mark

              S          Search preceding file as a library

              $Cd        Destination of console messages
                         d can be X (console), Y (printer),
                         or Z (zero output).  Default is X.

              $Id        Source of intermediate files;
                         d is disk drive A-P. Default
                         is current drive.

              $Ld        Source of library files;
                         d is disk drive A-P.  Default
                         is current drive.

              $Od        Destination of of object file;
                         d can be Z or disk drive A-P.
                         Default is to same drive as
                         first file in the LINK-80 command.

              $Sd        Destination of symbol file;
                         d can be Y or Z or disk drive A-P.
                         Default is to same drive as
                         first file in LINK-80 command.

    HELP>