      LINK

        EXAMPLES

      A>LINK b:MYFILE[NR]

           LINK-80 on drive A uses as input MYFILE.REL on drive B   and
           produces   the  executable  machine  code file MYFILE.COM on
           drive B.  The [NR] option specifies no symbol table file.

      A>LINK m1,m2,m3

           LINK-80 combines the separately compiled files m1,  m2,  and
           m3,  resolves  their  external  references, and produces the
           executable machine code file m1.COM.

      A>LINK m=m1,m2,m3

           LINK-80 combines the separately compiled files m1,  m2,  and
           m3 and produces the executable machine code file m.COM.

      A>LINK MYFILE,FILE5[s]

           The [s] option tells LINK-80 to search FILE5 as a   library.
           LINK-80    combines    MYFILE.REL    with   the   referenced
           subroutines contained in FILE5.REL  on  the  default   drive
           A  and  produces MYFILE.COM on drive A.

    HELP>