*********************************************************************** 
ATI Display Driver v3.098 for Windows 3.1x                 May 30, 1997

*********************************************************************** 
 
PLEASE READ THIS FILE COMPLETELY BEFORE ATTEMPTING TO USE THIS PRODUCT! 

***********************************************************************

Contents

1.0     Introduction
2.0     Installation Notes
3.0     ATI Contact Information

*****************************

1.0     Introduction

The mach64 device drivers supplied here are for Windows 3.1 and 
Windows 3.11. 

THIS SELF-EXTRACTING FILE CONTAINS DISPLAY DRIVER FILES ONLY.

*****************************

2.0     Installation Notes

IF YOU HAVE NOT INSTALLED A mach64 WINDOWS DRIVER PREVIOUSLY, YOU MAY 
REQUIRE YOUR MICROSOFT WINDOWS DISKETTES TO COMPLETE THE INSTALLATION 
OF THIS DRIVER.  

1. Exit Windows completely, and perform the following operations in DOS.
   Do NOT attempt to perform the driver installation from within 
   Windows.  

2. Run W31-3098.EXE from the directory it was downloaded into.  For this 
   example we will say W31-3098.EXE is located in C:\ATITEMP.
   eg.  CD ATITEMP        ;press enter
        W31-3098.EXE     ;press enter

3. Follow the screen prompts for installing the Windows 3.1 driver.  

4. LOAD64.EXE will be run from C:\ATI\SUPPORT\WIN31 after the installation
   files have been uncompressed.  This program is used to install the
   drivers into Windows 3.1X.  

   IF YOU RECEIVE AN ERROR MESSAGE, INDICATING THAT A CERTAIN FONT 
   (.fon) FILE IS NOT PRESENT, YOU WILL NEED TO RUN WINDOWS SETUP FROM
   DOS TO COMPLETE THE INSTALLATION.  WINDOWS SETUP WILL PROMPT YOU FOR
   THE DISKS ON WHICH THESE FONT FILES ARE FOUND.

   NOTE:  Windows 3.1X will default to a resolution of 640 X 480 with
          256 colors each time the mach64 driver is installed.

After successfully installing the ATI Display Driver, you can delete the 
contents of the directory C:\ATI\SUPPORT\WIN31 using UNSTALL.EXE.

We recommend that you keep a copy of W31-3098.EXE in case you need to 
install the driver again.


*****************************

3.0     ATI Contact Information

 Telephone numbers: 
   (905) 882-2600               Head Office, Sales and Marketing
   (905) 882-2620               Corporate Fax
   (905) 882-2626               Technical Support Voice
   (905) 882-0546               Technical Support Fax 
 Email:
   76004.3656@compuserve.com    Electronic Marketing
   74740,667                    Technical Support Compuserve
   support@atitech.ca           Technical Support Internet
 Driver Download Sites:
   www.atitech.ca               World Wide Web
   support.atitech.ca           Tech Support World Wide Web
   ftp.atitech.ca               FTP Download
   (905) 764-9404               BBS Download
   [GO] ATITECH                 Compuserve Forum
*****************************