#
# XXXXX IBM RAID Controller Support Diskette txtsetup.oem.
# NT 1/10/1994
#


[Disks]
#
# This section lists all disks in the disk set.
#
# <description> is a descriptive name for a disk, used when
#   prompting for the disk
# <tagfile> is a file whose presence allows setup to recognize
#   that the disk is inserted.
# <directory> is where the files are located on the disk.
#
d1 = "IBM RAID Controller Support Diskette", \ibmraidn, \nt


[Defaults]

# This section lists the default selection for each 'required'
# hardware component.  If a line is not present for a component,
# the default defaults to the first item in the [<component_name>]
# section (see below).
#
# <component_name> is one of computer, display, keyboard, mouse, scsi
# <id> is a unique <within the component> string to be associated
#   with an option.

scsi = OEMSCSI



[scsi]

# This section lists the options available for a particular component.
#
# <id> is the unique string for the option
# <description> is a text string, presented to the user in a menu


OEMSCSI = "IBM RAID Controller"



[Files.scsi.OEMSCSI]

# This section lists the files that should be copied if the user
# selects a particular component option.
#
# <file_type> is one of driver, port, class, dll, hal, inf, or detect.
#   See below.
# <source_disk> identifies where the file is to be copied from, and must
#   match en entry in the [Disks] section.
# <filename> is the name of the file. This will be appended to the
#   directory specified for the disk in the [Disks] section to form the
#   full path of the file on the disk.

driver = d1, ibmraidn.sys, Dac960Nt



[Config.Dac960Nt]
value = "", Tag, REG_DWORD, 99

